Other fluorescent lamp

means low pressue mercury electric-discharge sources in which a fluorescing coating transforms some of the ultraviolet energy generated by the mercury discharge into light and include circline lamps and include double-ended lamps with the following characteristics: Lengths from one to eight feet; designed for cold temperature applications; designed for use in reprographic equipment; designed to produce radiation in the ult ra-violet region of the spectrum; impact-resistant; reflectorized or aperture; or a CRI of 87 orgreater.