Automatic vent damper

means a device intended for installation in the venting system of an individual, automatically operated, fossil fuel‐fired appliance either in the outlet or downstream of the appliance draft control device, which is designed to automatically open the venting system when the appliance is in operation and to automatically close off the venting system when the appliance is in a standby or shutdown condition.