GU‐24s

means the designation of a lamp holder and socket configuration, based on a coding system by the International Energy Consortium: “G” indicates the broad type of two or more projecting contacts, such as pins or posts; “U” distinguishes between lamp and holder designs of similar type that are not interchangeable due to electrical or mechanical requirements; and “24” indicates 24 millimeter center to center spacing of electrical contact posts.”