Colored fluorescent lamps

means a fluorescent lamp designated and marketed as a colored lamp, and not designed or marketed for general illumination applications with either of the following characteristics:

(1) a CRI less than 40, as determined according to the method given in CIE publication 13.3‐ 1995, or

(2) a correlated color temperature less than 2,500K or greater than 7,000K as determined according to the method set forth in IES LM‐9‐09.