State-regulated small diameter directional lamp

means a directional lamp that meets all of the following criteria:

1. Capable of operating at 12 volts, 24 volts, or 120 volts;

2. Has an ANSI ANSLG C81.61-2009 (R2014) compliant pin base or E26 base;

3. Is a non-tubular directional lamp with a diameter of less than or equal to 2.25 inches;

4. Has a lumen output of less than or equal to 850 lumens, or has a wattage of 75 watts or less; and

5. Has a rated life greater than 300 hours.