NEMA Design C motor

means a squirrel-cage motor that:

(1) is Designed to withstand full-voltage starting and developing locked-rotor torque for high-torque applications up to the values shown in NEMA MG1-2009, paragraph 12.38.2);

(2) has pull-up torque not less than the values shown in NEMA MG1-2009, paragraph 12.40.2;

(3) has breakdown torque not less than the values shown in NEMA MG1-2009, paragraph 12.39.2;

(4) has a locked-rotor current not to exceed the values shown in NEMA MG1-2009, paragraphs 12.35.1 for 60 hertz and 12.35.2 for 50 hertz; and

(5) has a slip at rated load of less than 5 percent.