Refrigerator‐freezers

means a cabinet u sed with one or more doors, that has a source of refrigeration that requires single-phase, alternating current electric energy input only and consists of two or more compartments where at least one of the compartments is capable of maintaining compartment temperatures above 32oF (0oC) and below 39oF (3.9oC) as determined according to 10 C.F.R. section 429.14(d)(2), and at least one other compartment is capable of maintaining compartment temperatures of 8oF (-13.3oC) and may be adjusted by the user to a temperature of 0oF (-17.8oC) or below as determined according to 10 C.F.R. section 429.14(d)(2). However, the term does not include:

(1) Any product that does not include a compressor and condenser unit as an integral part of the cabinet assembly; or

(2) Any miscellaneous refrigeration product that must comply with an applicable miscellaneous refrigeration product energy conservation standard.