Built-in cooler

means any cooler with a total refrigerated volume of 7.75 ft3 or greater and no more than 24 inches in depth, excluding doors, handles, and custom front panels; that is designed, intended, and marketed exclusively to be:

(1) installed totally encased by cabinetry or panels that are attached during installation;

(2) securely fastened to adjacent cabinetry, walls or floor;

(3) equipped with unfinished sides that are not visible after installation; and

(4) equipped with an integral factory-finished face or built to accept a custom front panel.