Cooler-refrigerator-freezer

means a cabinet, used with one or more doors, that has a source of refrigeration that requires single-phase, alternating current electric energy input only, and consists of three or more compartments, including at least one cooler compartment as defined in 10 C.F.R. part 430, 430.27 where:

(1) At least one of the remaining compartments is not a cooler compartment as defined in 10 C.F.R. part 430, Appendix A of subpart B and is capable of maintaining compartment temperatures above 32oF (0oC) and below 39oF (3.9oC) as determined according to 10 C.F.R. section 429.61(d)(2); and

(2) At least one other compartment is capable of maintaining compartment temperatures below 8oF (-13.3oC) and may be adjusted by the user to a temperature of 0oF (-17.8oC) or below as determined according to 10 C.F.R. section 429.61(d)(2).