State-regulated compressor

means commercial and industrial equipment that meets all of the following criteria:

(1) is an air compressor,

(2) is a rotary compressor,

(3) is not a liquid-ring compressor,

(4) is driven by a brushless electric motor,

(5) is a lubricated compressor,

(6) has a full-load operating pressure greater than or equal to 75 pounds per square inch gauge (psig) and less than or equal to 200 psig,

(7) is not designed and tested to the requirements of The American Petroleum Institute standard 619, “Rotary-Type Positive-Displacement Compressors for Petroleum, Petrochemical, and Natural Gas Industries,”

(8) has full-load actual volume flow rate greater than or equal to 35 cubic feet per minute (cfm), or is sold or offered for sale with a compressor motor nominal horsepower greater than or equal to 10 horsepower (hp),

(9) has a full-load actual volume flow rate less than or equal to 1,250 cfm, or is sold or offered for sale with a compressor motor nominal horsepower less than or equal to 200 hp,

(10) is driven by a three-phase electric motor,

(11) is manufactured alone or as a component of another piece of equipment; and

(12) is one of the equipment classes listed in Table S-6.