Shatter‐resistant lamp, shatter‐proof lamp, or shatter‐protected lamp

means a lamp that:

(1) has a coating or equivalent technology that is compliant with the NSF/ANSI 51 and is designed to contain the glass if the glass envelope of the lamp is broken; and

(2) is designated and marketed for the intended application, with:

(A) the designation on the lamp packaging; and

(B) marketing material that identify the lamp as being shatter‐resistant, shatter‐proof, or shatter‐protected.