IEC Design H motor

means an electric motor that:

(1) is an induction motor designed for use with three-phase power;

(2) contains a cage rotor;

(3) is capable of direct-on-line starting

(4) has 4, 6, or 8 poles;

(5) is rated from 0.4 kW to 1600 kW at a frequency of 60 Hz; and

(6) conforms to sections 8.1, 8.2, and 8.3 of the IEC 60034-12 edition 2 requirements for starting torque, locked rotor apparent power, and starting.