Integral controls

means a fully functional occupancy sensor or automatic daylight control system for which all required components for an integral control, including control devices, sensors, and wiring, are factory installed, packaged and sold with each individual luminaire, and are integrated into each individual luminaire at the factory in one of the following three methods:

(1) Is integrated directly into the luminaire housing and hardwired to the lighting system; or

(2) Is pre‐wired to allow proper functionality between the control and luminaire, and to allow remote mounting of the control. One end of the wiring shall be pre‐wired to the luminaire, and the other end shall be prewired to the control. The wiring may be either a metal or fiber conductor. The wiring may allow temporary disconnection in the field to allow remote mounting of the control; or

(3) Is pre‐wired with a wireless radio controlled sensor to allow proper functionality between the control and luminaire, and to allow interaction with the wireless control signal in the lighting system.