## Section 1605.1. Federal and State Standards for Federally-Regulated Appliances.

### (a) Refrigerators, Refrigerator-Freezers, and Freezers.

(1) ‘Non‐Commercial Refrigerators, Non‐Commercial Refrigerator‐Freezers, and Non‐Commercial Freezers.

(A) The energy consumption of non‐‘commercial refrigerators designed for the refrigerated storage of food at temperatures above 32°F and below 39°F, configured for general refrigerated food storage, non‐commercial refrigerator‐freezers, and non‐commercial freezers, including drawer units, and kitchen units shall be not greater than the applicable values shown in Table A‐2. The standards shown in Table A-2 do not apply to non-commercial refrigerators and non-commercial refrigerator-freezers with total refrigerated volume exceeding 39 ft3 or non-commercial freezers with total refrigerated volume exceeding 30 ft3.

####

#### Table A-2
Standards for Non-Commercial Refrigerators, Refrigerator-Freezers, and Freezers

Product Class | Maximum Energy Use (kWh/year)* Equation
1. Refrigerator-freezers and refrigerators other than all-refrigerators with manual defrost | 7.99AV + 225.0 0.282av+ 225.0
1A. All-refrigerators -- manual defrost | 6.79AV + 193.6 0.240av + 193.6
2. Refrigerator-freezers—partial automatic defrost | 7.99AV + 225.0 0.282av+ 225.0
3. Refrigerator-freezers—automatic defrost with top-mounted freezer without an automatic icemaker | 8.07AV + 233.7 0.285av + 233.7
3-Bl. Built-in refrigerator-freezers---automatic defrost with top-mounted freezer without an automatic icemaker | 9.15AV + 264.9 0.323av + 264.9
3l. Refrigerator-freezers---automatic defrost with top-mounted freezer with an automatic icemaker without through-the-door ice service | 8.07AV + 317.7 0.285av + 317.7
3l-Bl Built-in refrigerator-freezers--automatic defrost with top-mounted freezer with an automatic icemaker without through-the-door ice service | 9.15AV + 348.9 0.323av + 348.9
3A. All refrigerators—automatic defrost | 7.07AV + 201.6 0.250av + 201.6.0
3A-Bl. Built-in All refrigerators—automatic defrost | 8.02AV + 228.5 0.283av + 228.5
4. Refrigerator-freezers--automatic defrost with side-mounted freezer without an automatic icemaker | 8.51AV + 297.8 0.301av + 297.8
4-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer without an automatic icemaker | 10.22AV + 357.4 0.361av + 357.4
4l. Refrigerator-freezers automatic defrost with side-mounted freezer with an automatic icemaker without through-the-door ice service | 8.51AV + 381.8 0.301av + 381.8
4l-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer with an automatic ice maker without through-the-door ice service | 10.22AV + 441.4 0.361av + 441.4
5. Refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker | 8.85AV + 317.0 0.312av + 317.0
5-Bl. Built-in refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker | 9.40AV + 336.9 0.332av + 336.9
5l. Refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker without through-the-door ice service. | 8.85AV + 401.0 0.312av + 401.0
5l-Bl. Built-in refrigerator-freezers automatic defrost with bottom-mounted freezer without an automatic icemaker without through-the-door ice service. | 9.40AV + 420.9 0.332av + 420.9
5A. Refrigerator-freezer automatic defrost with bottom-mounted freezer with through-the-door ice service. | 9.25AV + 475.4 0.327av + 475.4
5A-Bl. Built-in refrigerator-freezersautomatic defrost with bottom-mounted freezer with through-the-door ice service. | 9.83AV + 499.9 0.347av + 499.9
6. Refrigerator-freezers automatic defrost with top-mounted freezer with through-the-door ice service. | 8.40AV + 385.4 0.297av + 385.4
7. Refrigerator-freezers automatic defrost with side-mounted freezer with through-the-door ice service. | 8.54AV + 432.8 0.302av + 432.8
7-Bl. Built-in refrigerator-freezers automatic defrost with side-mounted freezer with through-the-door ice service. | 10.25AV + 502.6 0.362av + 502.6
8. Upright freezers with manual defrost | 5.57AV + 193.7 0.197av + 193.7
9. Upright freezers with automatic defrost without an automatic icemaker | 8.62AV + 228.3 0.305av + 228.3
9l. Upright freezers with automatic defrost with an automatic icemaker | 8.62AV + 312.3 0.348av + 260.9
9-Bl. Built-in upright freezers with automatic defrost without an automatic icemaker | 9.86AV + 260.9 0.348av + 260.9
9l-Bl. Built-in upright freezers with automatic defrost with an automatic icemaker | 9.86AV + 344.9 0.348av + 344.9
10. Chest freezers and all other freezers except compact freezers | 7.29AV + 107.8 0.257av + 107.8
10A. Chest freezers with automatic defrost | 10.24AV + 148.1 0.362av + 148.1
11. Compact refrigerator-freezers and refrigerators other than all-refrigerators with manual defrost | 9.03AV + 252.3 0.319av + 252.3
11A. Compact all refrigerators---manual defrost | 7.84AV + 219.1 0.277av + 219.1
12. Compact refrigerator-freezers--partial automatic defrost | 5.91AV + 335.8 0.209av + 335.8
13. Compact refrigerator-freezers--automatic defrost with top-mounted freezer | 11.80AV + 339.2 0.417av + 339.2
13l. Compact refrigerator-freezers--automatic defrost with top-mounted freezer with an automatic icemaker | 11.80AV + 423.2 0.417av + 423.2
13A. Compact all refrigerators---automatic defrost | 9.17AV + 259.3 0.324av + 259.3
14. Compact refrigerator-freezers--automatic defrost with side-mounted freezer | 6.82AV + 456.9 0.241av + 456.9
14l. Compact refrigerator-freezers--automatic defrost with side-mounted freezer with an automatic icemaker | 6.82AV + 540.9 0.241av + 540.9
15. Compact refrigerator-freezers--automatic defrost with bottom-mounted freezer | 11.80AV + 339.2 0.417av + 339.2
15l. Compact refrigerator-freezers--automatic defrost with bottom-mounted freezer with an automatic icemaker | 11.80AV + 423.2 0.417av + 423.2
16. Compact upright freezers with manual defrost | 8.65AV + 225.7 0.306av + 225.7
17. Compact upright freezers with automatic defrost | 10.17AV + 351.9 0.359av + 351.9
18. Compact chest freezers | 9.25AV + 136.8 0.327av + 136.8
*AV = Adjusted total Volume, Expressed in ft3, as determined in 10 C.F.R. sections 430.23(a) (Appendix A to subpart B of part 430) and 430.23(b) (Appendix B to subpart B of part 430) *av = Adjusted total volume, expressed in Liters.

(B) Miscellaneous refrigeration products. The energy standards as determined by the equations shown in Table A-3 shall be rounded off to the nearest kWh per year. If the equation calculation is halfway between the nearest two kWh per year values, the standard shall be rounded up to the higher of these values.

1. Coolers manufactured on or after October 28, 2019 shall have Annual Energy Use (AEU) not more than the applicable values shown in Table A-3.

#### Table A-3
Standards for Miscellaneous Refrigeration Products

Product Class | Maximum Annual Energy Use (AEU) (kWh/Year)
Coolers
Built-in Compact Cooler | 7.88Av + 155.8
Built-in Cooler
Freestanding Compact Cooler
Freestanding Cooler
Combination Coolers
Combination Cooler with all refrigerator-automatic defrost | 4.57AV + 130.4
Built-in combination cooler with all refrigerator-automatic defrost | 5.19AV + 147.8
Combination Cooler with upright freezers with automatic defrost without an automatic icemaker | 5.58AV + 147.7
Built-in combination cooler with upright freezer with automatic defrost without an automatic icemaker | 6.38AV + 168.8
Combination Cooler with upright freezer with automatic defrost with an automatic icemaker | 5.58AV + 231.7
Built-in combination cooler with upright freezer with automatic defrost with an automatic icemaker | 6.38AV + 252.8
Compact combination cooler with all refrigerator-automatic defrost | 5.93AV + 193.7
Built-in compact combination cooler with all refrigerator-automatic defrost | 6.52AV + 213.1
AV= Adjusted total volume, expressed in ft3, as calculated according to 10 C. F. R. Appendix A to subpart B of part 430.

(2) Commercial Refrigerators, Commercial Refrigerator-Freezers, and Commercial Freezers.

(A) The daily energy consumption (in kilowatt hours per day) of each commercial ‘refrigerator and commercial freezer manufactured on or after March 27, 2017 shall be not greater than the applicable values shown in Tables A-4, A-5, and A-6.

#### Table A-4
Standards for Commercial Refrigerators, and-Freezers
with a Self-Contained Condensing Unit That are Not Commercial Hybrid Units

Equipment Category | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers | Self Contained (SC) | Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, SC, M VCT, SC, L | 0.1 × V + 0.86 0..29 × V + 2.95
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, SC, M VCS, SC, L | 0.05 × V + 1.36 0.22 × V + 1.38
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, SC, M HCT, SC, L | 0.06 × V + 0.37 0.08 × V + 1.23
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, SC, M HCS, SC, L | 0.05 × V + 0.91 0.06 × V + 1.12
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, SC, M SOC, SC, L | 0.51 x TDA + 1.0 1.10 × TDA + 2.10
Refrigerators with transparent doors | Self Contained (SC) | Pull Down PD) | 38 (P) | ≥ 32 | PD, SC, M | 0.11 × V + 0.81
Refrigerators and Freezers without Doors | Self Contained (SC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, SC, M VOP, SC, L | 1.69 × TDA + 4.71 4.25 × TDA +11.82
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, SC, M SVO, SC, L | 1.70 × TDA + 4.59 4.26 × TDA +11.51
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, SC, M HZO, SC, L | 0.72 × TDA + 5.55 1.90 × TDA + 7.08
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.

#### Table A-5
Standards for Commercial Refrigerators and Freezers
with a Remote Condensing Unit That are Not Commercial Hybrid Units

Equipment Category | Condensing Unit Configuration | Equipment Family | Rating Temperature (°F) | Operating Temperature (°F) | Equipment Class Designation* | Maximum Daily Energy Consumption (kWh)
Refrigerators and Freezers | ‘Remote (RC) | Vertical Open (VOP) | 38 (M) 0 (L) | ≥ 32 < 32 | VOP, RC, M VOP, RC, L | 0.64 × TDA + 4.07 2.20 × TDA + 6.85
Semivertical Open (SVO) | 38 (M) 0 (L) | ≥ 32 < 32 | SVO, RC, M SVO, RC, L | 0..66 × TDA + 3.18 2.20 × TDA + 6.85
Horizontal Open (HZO) | 38 (M) 0 (L) | ≥ 32 < 32 | HZO, RC, M HZO, RC, L | 0.35 × TDA + 2.88 0.55 × TDA + 6.88
Vertical Closed Transparent (VCT) | 38 (M) 0 (L) | ≥ 32 < 32 | VCT, RC, M VCT, RC, L | 0..15 × TDA + 1.95 0.49 × TDA + 2.61
Horizontal Closed Transparent (HCT) | 38 (M) 0 (L) | ≥ 32 < 32 | HCT, RC, M HCT, RC, L | 0.16 × TDA + 0.13 0.34 × TDA + 0.26
Vertical Closed Solid (VCS) | 38 (M) 0 (L) | ≥ 32 < 32 | VCS, RC, M VCS, RC, L | 0.10 × V + 0.26 0.21 × V + 0.54
Horizontal Closed Solid (HCS) | 38 (M) 0 (L) | ≥ 32 < 32 | HCS, RC, M HCS, RC, L | 0.10 × V + 0.26 0.21 × V + 0.54
Service Over Counter (SOC) | 38 (M) 0 (L) | ≥ 32 < 32 | SOC, RC, M SOC, RC, L | 0..44 × TDA + 0.11 0.93 × TDA + 0.22
* The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family, and Rating Temperature (°F) columns to the left.

(B) The daily energy consumption (in kilowatt hours per day) of commercial ice cream freezer that are not commercial hybrid units and that are manufactured on or after March 27, 2017, shall be not greater than the applicable values shown in Table A‐6.

#### Table A-6
Standards for Commercial Ice Cream Freezers That are Not Commercial
Hybrid Units and Are Manufactured on or After March 27, 2017

Equipment Family | Condensing Unit Configuration | Equipment Class Designation1 | Maximum Daily Energy Consumption (kWh)2
Vertical Open (VOP) | ‘Remote (RC) Self‐Contained (SC) | VOP, RC, I VOP, SC, I | 2.79 × TDA + 8.7 5.40 × TDA +15.02
Semivertical Open (SVO) | ‘Remote (RC) Self‐Contained (SC) | SVO, RC, I SVO, SC, I | 2.79 × TDA + 8.7 5.41 × TDA +14.63
Horizontal Open (HZO) | ‘Remote (RC) Self‐Contained (SC) | HZO, RC, I HZO, SC, I | 0.70 × TDA + 8.74 2.42 × TDA + 9
Vertical Closed Transparent (VCT) | Remote (RC) Self‐Contained (SC) | VCT, RC, I VCT, SC, I | 0.58 × TDA + 3.05 0.62 × TDA + 3.29
Horizontal Closed Transparent (HCT) | ‘Remote (RC) Self‐Contained (SC) | HCT, RC, I HCT, SC, I | 0.40 × TDA + 0.31 0.56 × TDA + 0.43
Vertical Closed Solid (VCS) | ‘Remote (RC) Self‐Contained (SC) | VCS, RC, I VCS, SC, I | 0.25 × V + 0.63 0.34 × V + 0.88
Horizontal Closed Solid (HCS) | ‘Remote (RC) Self‐Contained (SC) | HCS, RC, I HCS, SC, I | 0.25 × V + 0.63 0.34 × V + 0.88
Service Over Counter (SOC) | ‘Remote (RC) Self‐Contained (SC) | SOC, RC, I SOC, SC, I | 1.09 × TDA + 0.26 1.53 × TDA + 0.36
1 The meaning of the letters in this column is indicated in the Condensing Unit Configuration, Equipment Family and Rating Temperature (oF) columns to the left, and where “I” respresents “ice cream freezer.” 2 Based on Rating Temperature ‐15°F and Operating Temperature ≤ ‐5°F.

(C) Commercial refrigeration equipment with two or more compartments. For commercial refrigeration equipment with two or more compartments, (i.e., hybrid ‘refrigerators, hybrid ‘freezers, hybrid ‘refrigerator‐freezers, and non‐hybrid ‘refrigerator‐freezers), the maximum daily energy consumption (MDEC) for each model shall be the sum of the MDEC values for all of its compartments. For each compartment, measure the TDA or volume of that compartment, and determine the appropriate equipment class based on that compartment’s equipment family, condensing unit configuration, and designed operating temperature. The MDEC limit for each compartment shall be the calculated value obtained by entering that compartment’s TDA or volume into the standard equation in Table A-4, Table A-5 or Table A-6 of this Article for that compartment’s equipment class. Measure the calculated daily energy consumption (CDEC) or total daily energy consumption (TDEC) for the entire case as described in 10 C.F.R. section 431.66(d)(2)(i) through(iii), except that where measurements and calculations reference ARI Standard 1200-2006, AHRI Standard 1200 (I-P)-2010 shall be used.

(D) ‘Wedge Cases. For remote‐condensing and self‐contained wedge cases, measure the CDEC or TDEC according to the ARI Standard 1200 (I-P)-2010 test procedure incorporated by reference in 10 C.F.R. section 431.63. For wedge cases in equipment classes for which a volume metric is used, the MDEC shall be the amount derived from the appropriate standards equation in Table A-4, Table A-5, or Table A-6 of this Article. For wedge cases of equipment classes for which a TDA metric is used, the MDEC for each model shall be the amount derived by incorporating into the standards equation in Table A-4, Table A-5, or Table A-6 of this Article for the appropriate equipment class a value for the TDA that is the product of:

1. The vertical height of the air-curtain (or glass in a transparent door), and

2. The largest overall width of the case, when viewed from the front.

Exception: to Section 1605.1(a)(2) of this Article: The standards shown in section 1605.1(a)(2) of this Article do not apply to salad bars, buffet tables, chef bases, or griddle stands.

(3) ‘Automatic Commercial Ice Makers.

(A) Cube Type. Each cube type ‘automatic commercial ice maker with capacities between 50 and 2500 pounds per 24-hour period and is manufactured on or after January 1, 2010, and before January 28, 2018, shall meet the standard levels set forth in Table A-7.

#### Table A-7
Standards for Cube Type Automatic Commercial Ice Makers
Manufactured on or After January 1, 2010 and Before January 28, 2018

Equipment type | Type of cooling | Harvest rate (lbs ice /24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (gal/100 lbs ice)
Ice Making Head | Water | < 500 | 7.80–0.0055H | 200–0.022H.
≥ 500 and < 1436 | 5.58–0.0011H | 200–0.022H.
≥ 1436 | 4.0 | 200–0.022H.
Ice Making Head | Air | < 450 | 10.26–0.00 86H | Not applicable.
≥ 450 | 6.89-0.0011H | Not applicable.
Remote Condensing (but not remote compressor) | Air | < 1000 | 8.85–0.0038H | Not applicable.
≥ 1000 | 5.1 | Not applicable.
Remote Condensing and R emote C ompressor) | < 934 | 8.85–0.0038H | Not applicable.
≥ 934 | 5.3 | Not applicable.
Self Contained | Water | < 200 | 11.40-0.019H | 191–0.0315H.
≥ 200 | 7.6 | 191–0.0315H.
Self Contained | Air | < 175 | 18.0–0.0469H | Not applicable.
≥ 175 | 9.8 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

(B) Batch Type. Each batch type automatic commercial ice maker with capacities between 50 and 4000 pounds per 24-hour period and is manufactured on or after January 28, 2018, shall meet the standard levels set forth in Table A-8.

1. Batch type automatic commercial ice makers include cube type automatic commercial ice makers for purposes of the standards for models manufactured on or after January 28, 2018.

#### Table A-8
Standards for Batch Type Automatic Commercial Ice Makers
Manufactured on or After January 28, 2018

Equipment type | Type of cooling | Harvest rate (lbs ice/24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (galloons/100 lbs ice)
Ice Making Head | Water | ≥50 and < 300 | 6.88-0.0055H | 200–0.022H.
≥ 300 and < 850 | 5.80–0.00191H | 200–0.022H.
≥ 850 and< 1500 | 4.42-0.00028H | 200–0.022H.
≥ 1500 and < 2500 | 4.0 | 200–0.022H.
≥2500 and < 4000 | 4.0 | 145.
Air | ≥50 and < 300 | 10-0.01233H | Not applicable.
≥ 300 and < 850 | 7.05-0.0025H | Not applicable.
≥ 850 and< 1500 | 5.55-0.00063H | Not applicable.
≥ 1500 and < 4000 | 4.61 | Not applicable.
Remote Condensing (but not remote compressor) | Air | ≥ 50 and < 988 | 7.97-0.00342H | Not applicable.
≥ 988 and < 4000 | 4.59 | Not applicable.
Remote Condensing and Remote Compressor | ≥ 50 and < 930 | 7.97-0.00342H | Not applicable.
≥ 930 and < 4000 | 4.79 | Not applicable.
Self-Contained | Water | ≥ 50 and < 200 | 9.5-0.019H | 191–0.0315H.
≥ 200 and < 2500 | 5.7 | 191–0.0315H.
≥ 2500 and < 4000 | 5.7 | 112
Air | ≥ 50 and < 110 | 14.79-0.0469H | Not applicable.
≥ 110 and < 200 | 12.42-0.02533H | Not applicable.
≥ 200 and < 4000 | 7.35 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

(C) Continuous Type. Each continuous type ‘automatic commercial ice maker with capacities between 50 and 4,000 pounds per 24-hour period manufactured on or after January 28, 2018, shall meet the standard levels set forth in Table A-9.

#### Table A-9
Standards for Continuous Type Automatic Commercial Ice Makers
Manufactured on or After January 28, 2018

Equipment type | Type of cooling | Harvest rate (lbs ice/24 hours) | Maximum ‘energy use (kWh/100 lbs ice) | Maximum condenser water use* (gal/100 lbs ice)
Ice Making Head | Water | ≥50 and < 801 | 6.48-0.00267H | 180-0.0198H.
≥ 801 and < 2500 | 4.34 | 180-0.0198H.
≥ 2500 and< 4000 | 4.34 | 130.5
Air | ≥ 50 and < 310 | 9.19-0.00629H | Not applicable.
≥310 and < 820 | 8.23-0.0032H | Not applicable.
≥820 and < 4000 | 5.61 | Not applicable.
Remote Condensing (but not remote compressor) | Air | ≥ 50 and < 800 | 9.7-0.0058H | Not applicable.
≥ 800 and < 4000 | 5.06 | Not applicable.
Remote Condensing and Remote Compressor | ≥ 50 and < 800 | 9.9-0.0058H | Not applicable.
≥ 800 and < 4000 | 5.26 | Not applicable.
Self-Contained | Water | ≥ 50 and < 900 | 7.6-0.00302H | 153-0.0252H.
≥ 900 and < 2500 | 4.88 | 153-0.0252H.
≥ 2500 and < 4000 | 4.88 | 90
Air | ≥ 50 and < 200 | 14.22-0.03H | Not applicable.
≥ 200 and < 700 | 9.47-0.00624H | Not applicable.
≥ 700 and < 4000 | 5.1 | Not applicable.
H Harvest rate in pounds per 24 hours. *Water use is for the condenser only and does not include potable water used to make ice.

(4) Walk‐In Coolers and Walk‐In Freezers. Walk‐in coolers and walk‐in ‘freezers manufactured on or after January 1, 2009 shall:

(A) have automatic door closers that firmly close all walk‐in doors that have been closed to within one inch of full closure, except that this subparagraph shall not apply to doors wider than three feet nine inches or taller than seven feet;

(B) have strip doors, spring hinged doors, or other method of minimizing infiltration when doors are open;

(C) contain wall, ceiling, and door insulation of at least R‐25 for coolers and R‐32 for freezers, except that this subparagraph shall not apply to:

1. glazed portions of doors nor to structural members; and

2. A walk-in cooler or walk-in ‘freezer component if the component manufacturer has demonstrated to the satisfaction of the Secretary in a manner consistent with applicable requirements that the component reduces energy consumption at least as much as if such insulation requirements of Section 1605.1(a)(4)(C) of this Article were to apply.

(D) contain floor insulation of at least R‐28 for freezers;

(E) for evaporator fan motors of under one horsepower and less than 460 volts, use:

1. electronically commutated motors (brushless direct current motors); or

2. 3‐phase motors;

(F) for condenser fan motors of under one horsepower, use:

1. electronically commutated motors;

2. permanent split capacitor‐type motors; or

3. 3‐phase motors; and

(G) for all interior lights, use light sources with an efficacy of 40 lumens per watt (LPW) or more, including ballast losses (if any), except that light sources with an efficacy of 40 LPW or less, including ballast losses (if any), may be used in conjunction with a timer or device that turns off the lights within 15 minutes of when the walk‐in cooler or walk‐in freezer is not occupied by people.

(5) Walk‐In Coolers with Transparent Reach‐in Doors and Walk‐In Freezers with Transparent Reach‐In Doors. In ‘addition to the design standards in Section 1605.1(a)(4)of this Article, walk‐in coolers equipped with transparent reach‐in doors and walk‐in freezers equipped with transparent reach‐in doors and manufactured on or after January 1, 2009 shall also meet the following design standards:

(A) Transparent reach‐in doors for walk‐in freezers and windows in walk‐in freezer doors shall be of triple‐pane glass with either heat‐reflective treated glass or ‘gas fill;

(B) Transparent reach‐in doors for walk‐in coolers and windows in walk‐in cooler doors shall be either:

1. double‐pane glass with heat‐reflective treated glass and ‘gas fill; or

2. triple‐pane glass with either heat‐reflective treated glass or ‘gas fill;

(C) If the walk-in cooler or walk-in freezer has an anti-sweat heater

1. without anti-sweat heat controls, the walk in cooler or walk-in freezer shall have a total door rail, glass, and frame heater power draw of not more than 7.1 watts per square foot (W/ft2) of door opening (for freezers) and 3.0 watts per square foot (W/ft2) of door opening (for coolers);

2. with anti-sweat heat controls, and the total door rail, glass, and frame heater power draw is more than 7.1 watts per square foot (W/ft2) of door opening (for freezers) and 3.0 watts per square foot (W/ft2) of door opening (for coolers), the anti-sweat heat controls shall reduce the energy use of the anti-sweat heater in a quantity corresponding to the relative humidity in the air outside the door or to the condensation on the inner glass pane.

(D) Walk-in cooler and freezer display doors. All walk-in cooler and walk-in freezer display doors manufactured on or after June 5, 2017, must not exceed the standards shown in Table A-10:

#### Table A-10
Standards for Walk-in Cooler and Walk-in Freezer Display Doors
Manufactured On or After June 5, 2017

Class Descriptor | Class | Maximum Daily Energy Consumption (kWh/day)*
Display Door, Medium Temperature | DD.M | 0.04 X Add + 0.41
Display Door, Low Temperature | DD.L | 0.15 X Add + 0.29
*Add represents the surface area of the display door.

(E) Walk-in cooler and freezer non-display doors. All walk-in cooler and walk-in freezer non-display doors manufactured on or after June 5, 2017, must not exceed the standards shown in Table A-11:

#### Table A-11
Standards for Walk-in Cooler and Walk-in Freezer
Non-Display Doors Manufactured On or After June 5, 2017

Class Descriptor | Class | Maximum Daily Energy Consumption (kWh/day)*
Passage Door, Medium Temperature | PD.M | 0.05 X And + 1.7
Passage Door, Low Temperature | PD.L | 0.14 X And+ 4.8
Freight Door, Medium Temperature | FD.M | 0.04 X And + 1.9
Freight Door, Low Temperature | FD.L | 0.12 X And + 5.6
*And represents the surface area of the non-display door

(F) Walk-in cooler and freezer refrigeration systems. The annual walk-in energy factor of all walk-in cooler and walk-in freezer refrigeration systems manufactured on or after January 1, 2020, must not be less than the values shown in Table A-12:

#### Table A-12
Standards for Walk-in Cooler and Walk-in Freezer Refrigeration Systems
Manufactured On or After January 1, 2020

Class Descriptor | Class | Minimum AWEF (Btu/W-h
Dedicated Condensing, Medum Temperature, Indoor System | DC, M, I | 5.61
Dedicated Condensing, Medum Temperature, Outdoor System | DC, M, 0 | 7.60

(6) Refrigerated Canned and Bottled Beverage Vending Machines.

(A) Refrigerated Canned and Bottled Beverage Vending Machines Manufactured Before January 8, 2019. The daily energy consumption (in kilowatt hours per day) when measured at the 75°F ± 2°F and 45 ± 5% RH condition of each ‘refrigerated bottled or canned beverage vending machine manufactured on or after the effective dates shown shall be not greater than the values shown in Table A-13:

#### Table A-13
Standards for Refrigerated Canned and Bottled Beverage Vending Machines
Manufactured On or After August 31, 2012 and Before January 8, 2019

Equipment Class | Maximum Daily Energy Consumption (MDEC) (kWh)
Class A | 0.055 × V + 2.56
Class B | 0.073 × V + 3.16
Combination Vending Machines | RESERVED
V= Representative value of refrigerated volume in ft3

(B) Refrigerated Canned and Bottled Beverage Vending Machines Manufactured On or After January 8, 2019. The daily energy consumption (in kilowatt hours per day) of refrigerated canned and bottled beverage vending machines manufactured on or after January 8, 2019 shall not exceed the values shown in Table A-14:

#### Table A-14
Standards for Refrigerated Canned and Bottled Beverage Vending Machines
Manufactured on or After January 8, 2019

Equipment Class | Maximum Daily Energy Consumption (MDEC) (kWh)
Class A | 0.052 X V + 2.43
Class B | 0.052 X V + 2.20
Combination A | 0.086 X V + 2.66
Combination B | 0.111 X V + 2.04
V = Representative value of refrigerated volume in ft3

(7) Coolers Manufactured Before October 28, 2019, and Water Dispensers. See section 1605.3(a) of this Article for energy efficiency standards for:

(A) consumer refrigeration coolers manufactured before October 28, 2019; and

(B) water dispensers.

### (b) Room Air Conditioners, Room Air‐Conditioning Heat Pumps, Packaged Terminal Air Conditioners, and Packaged Terminal Heat Pumps.

(1) Room Air Conditioners and Room Air‐Conditioning Heat Pumps.

The combined EER of room air conditioners and room air-conditioning heat pumps that are manufactured on or after June 1, 2014 shall be not less than the applicable values shown in Table B-2. The EER of room air conditioners and room air-conditioning heat pumps that are labeled for use at more than one voltage shall be not less than the applicable values shown in Table B-2 at each of the labeled voltages.

#### Table B-2
Standards for Room Air Conditioners and Room Air-Conditioning
Heat Pumps Manufactured On or After June 1, 2014

Appliance | Louvered Sides | Cooling Capacity (Btu/hr) | Minimum Combined EER
Room ‘Air Conditioner | Yes | < 6,000 | 11.0
Room Air Conditioner | Yes | ≥ 6,000 – ≤7,999 | 11.0
Room Air Conditioner | Yes | ≥ 8,000 – ≤13,999 | 10.9
Room Air Conditioner | Yes | ≥ 14,000 – ≤19,999 | 10.7
Room Air Conditioner | Yes | ≥ 20,000 – ≤27,999 | 9.4
Room Air Conditioner | Yes | ≥ 28,000 | 9.0
Room Air Conditioner | No | < 6,000 | 10.0
Room Air Conditioner | No | ≥ 6,000 – ≤7,999 | 10.0
Room Air Conditioner | No | ≥ 8,000 – ≤10,999 | 9.6
Room Air Conditioner | No | ≥ 11,000 – ≤13,999 | 9.5
Room Air Conditioner | No | ≥ 14,000 – ≤9,999 | 9.3
Room Air Conditioner | No | ≥20,000 | 9.4
Room Air Conditioning Heat Pump | Yes | < 20,000 | 9.8
Room Air Conditioning Heat Pump | Yes | ≥20,000 | 9.3
Room Air Conditioning Heat Pump | No | < 14,000 | 9.3
Room Air Conditioning Heat Pump | No | ≥14,000 | 8.7
Casement‐Only Room Air Conditioner | Either | Any | 9.5
Casement‐Slider Room Air Conditioner | Either | Any | 10.4

(2) ‘Packaged Terminal Air Conditioners and ‘Packaged Terminal Heat Pumps.

The EER and COP, as applicable, of non-standard size packaged terminal air conditioners and non standard size packaged terminal heat pumps manufactured on or after October 7, 2010, and of standard size packaged terminal air conditioners and standard size packaged terminal heat pumps manufactured on or after January 1, 2017 shall be not less than the applicable values shown in Tables B-3 and B-4.

#### Table B-3
Standards for Non-Standard Size Packaged Terminal Air Conditioners
and Non-Standard Size Packaged Terminal Heat Pumps Manufactured On or after October 7, 2010

Appliance | Cooling Capacity (Btu/hr) | Minimum ‘Efficiency
Minimum EER | Minimum COP
Packaged terminal air conditioners | < 7,000 | 9.4 | —
> 7,000 and < 15,000 | 10.9 – (0.213 x Cap1) | —
> 15,000 | 7.7 | —
Packaged terminal ‘heat pumps | < 7,000 | 9.3 | 2.7
> 7,000 and < 15,000 | 10.8 – (0.213 x Cap1) | 2.9 ‐ (0.026 x Cap1)
> 15,000 | 7.6 | 2.5
1Cap means cooling capacity in thousand British thermal units per hour (Btu/h) at 95°F outdoor dry-bulb

#### Table B-4
Standards for Standard Size Packaged Terminal Air Conditioners and Standard Size Packaged
Terminal Heat Pumps Manufactured On or after January 1, 2017

Appliance | Cooling Capacity (Btu/hour) | Minimum ‘Efficiency
Minimum EER | Minimum COP
Packaged Terminal ‘Air Conditioners | < 7,000 | 11.9 |
≥ 7,000 < 15,000 | 14.0-(0.300 x Cap1) |
≥ 15,000 | 9.5 |
Packaged Terminal ‘Heat Pumps | < 7,000 | 11.9 | 3.3
≥ 7,000 < 15,000 | 14.0-(0.300 x Cap1) | 3.7 – (0.52 x Cap1)
≥ 15,000 | 9.5 | 2.9
1 Cap means cooling capacity in thousand British thermal units per hour (Btu/h) at 95°F outdoor dry‐ bulb temperature.

### (c) Central Air Conditioners, Air Filters, and Heat Pump Water-Heating Packages.

(1) ‘Central Air Conditioners. The EER, IEER, SEER, COP, HSPF, SCOP, ISCOP2, and ISMRE2 as applicable, of all central ‘air conditioners, including computer room air conditioners, shall be not less than the applicable values shown in Tables C‐3, C‐4, C‐5, C-6, C-7, C-8, C‐9, C-10 and C-11.

(A) Evaporatively Cooled ‘Computer Room Air Conditioners. See Section 1605.3(c) of this Article for energy ‘efficiency standards for evaporatively cooled computer room air conditioners.

#### Table C-3
Standards for Single Phase Air-Cooled Air Conditioners with Cooling Capacity
Less than 65,000 Btu per Hour and Single Phase Air-Source Heat Pumps
with Cooling Capacity Less than 65,000 Btu per Hour, Not Subject to EPAct, Manufactured on or After January 1, 2015, but Before January 1, 2023

Product Class | Minimum SEER | Minimum HSPF | Minimum EER | Average Off‐ Mode Power Consumption Pw. pff (watts)
Split system ‘air conditioners with rated cooling capacity < 45,000 Btu/hour¹ | 13.0 | — | 12.2 | 30
Split system air conditioners with rated cooling capacity ≥ 45,000 Btu/hour¹ | 13.0 | 11.7 | 30
Split system heat pumps | 14.0 | 8.2 |  | 33
Split system heat pumps with rated cooling capacity ≥ 45,000 Btu/hour¹ |  | 33
Single package air conditioners1 | 14.0 |  | 11.0 | 30
Single package heat pumps | 14.0 | 8.0 |  | 33
Space constrained air conditioners | 12.0 |  | — | 30
Space constrained heat pumps | 12.0 | 7.4 | — | 33
Small duct, high velocity ‘air conditioner systems | 12.0 | 7.2 | — | 30
Small duct, high velocity ‘heat pump systems | 12.0 | 7.2 | — | 30
1 Minimum SEER of 14.0 required for units installed on or after January 1, 2015, but before January 1, 2023, in the states of Alabama, Arkansas, Delaware, Florida, Georgia, Hawaii, Kentucky, Louisiana, Maryland, Mississippi, North Carolina, Oklahoma, South Carolina, Tennessee, Texas, or Virginia, or in the District of Columbia.

#### Table C-4
Standards for Air Conditioners and Heat Pumps That Are Consumer Products, Manufactured on or After January 1, 2023

Product Class | Minimum SEER2 | Minimum HPSF2 | Minimum EER21 | Maximum Average Off- Mode Power Consumption P w, pff (watts)2
Split system air conditioners with certified cooling capacity < 45,000 Btu/hour | 13.4/14.3* |  | 11.7/9.8** | 30
Split system air conditioners with certified cooling capacity ≥ 45,000 Btu/hour | 13.4/13.8* |  | 11.2/9.8*** | 30
Split system heat pumps | 14.3 | 7.5 |  | 33
Single package air conditioners | 13.4 |  | 10.6 | 30
Single package heat pumps | 13.4 | 6.7 |  | 33
Small duct, high velocity air conditioner systems | 12.0 | 6.1 |  | 30
Small duct, high velocity heat pump systems | 12.0 | 6.1 |  | 30
Space constrained air conditioners | 11.7 |  |  | 30
Space constrained heat pumps | 11.9 | 6.3 |  | 33
¹ Minimum EER2 standards for units that are installed in the Southwest (Arizona, California, Nevada, or New Mexico). 2 Maximum Average Off-Mode Power Consumption standard applies to units manufactured on or after January 1, 2015. * The higher minimum SEER2 standard applies to units that are installed in the Southwest. See 10 C.F.R. section 430.32(c) for less stringent federal standards applicable to these units that are manufactured on or after January 1, 2023, and installed in states other than the Southwest. ** The 11.7 EER2 standard applies to products with a certified SEER2 less than 15.2. The 9.8 EER2 standard applies to products with a certified SEER2 greater than or equal to 15.2. *** The 11.2 EER2 standard applies to products with a certified SEER2 less than 15.2. The 9.8 EER2 standard applies to products with a certified SEER2 greater than or equal to 15.2.

EXCEPTION to Section 1605.1(c)(1) Table C-5 of this Article: The standards shown in Table

C-5 do not apply to single package vertical air conditioners and single package vertical heat

pumps (see Table C-7), packaged terminal air conditioners and packaged terminal heat

pumps (see Tables B-3 and B-4), computer room air conditioners (see Table C-8), variable

refrigerant flow multi-split air conditioners and heat pumps (see Table C-9), and double-duct

air-cooled commercial package air conditioning and heating equipment (see Table C-10).

#### Table C-5
Standards for Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled) Air Conditioners and Air-Source Heat Pumps Subject to EPAct
(Standards Effective January 1, 2010 do not apply to Single Package Vertical Air Conditioners)

Equipment Type | Cooling Capacity | Sub-category | Heating Type* | Efficiency Levels | Compliance date: Equipment Manufactured starting on
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled, 3-Phase, Split-System) | < 65,000 Btu/h | AC | ALL | SEER = 13.0 | June 16, 2008
HP | SEER = 14.0 HSPF = 8.2 | January 1, 2017
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled, 3-Phase, Single-Package) | < 65,000 Btu/h | AC | ALL | SEER = 14.0 | January 1, 2017
HP | SEER = 14.0 HSPF = 8.0 | January 1, 2017
Small Commercial Package Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 65,000 Btu/h and < 135,000 Btu/h | AC | N-E | EER = 11.2 | January 1, 20101
IEER = 12.9 | January 1, 20182
IEER = 14.8 | January 1, 2023
A-O | EER = 11.0 | January 1, 20101
IEER = 12.7 | January 1, 20182
IEER = 14.6 | January 1, 2023
HP | E-N |
EER = 11.0 COP = 3.3
IEER = 12.9 COP = 3.3
IEER = 14.8 COP = 3.4
| January 1, 20101
January 1, 20182
January 1, 2023
A-O |
EER = 10.8 COP = 3.3
IEER = 12.0 COP = 3.3
IEER = 13.9 COP = 3.4
| January 1, 20101
January 1, 20182
January 1, 2023

#### Table C-6
Standards for Commercial Package Air Conditioning and Heating Equipment (Water-Cooled) Air Conditioners, Commercial Package Air Conditioning and Heating Equipment (Evaporatively Cooled) Air Conditioners, and Small Commercial Package Water-Source Heat Pumps

Equipment Type | Cooling Capacity | Subcategory | Heating Type* | Efficiency Levels | Compliance date: Equipment manufactured starting on

Small Commercial Package Air Conditioning and Heating Equipment (Water-Cooled) | < 65,000 Btu/h | AC | All | EER = 12.1 | October 29, 2003

N-E A-O | EER = 12.1 EER = 11.9
≥65,000 Btu/h and < 135,000 Btu/h | June 2, 2013

Large Commercial Package Air-Conditioning and Heating Equipment (Water-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | N-E A-O | EER = 12.5 EER = 12.3 | June 2, 2014 |
Very Large Commercial Package Air-Conditioning and Heating Equipment (Water-Cooled) | ≥ 240,000 Btu/h and < 760,000 Btu/h | AC | N-E A-O | EER = 11.9 EER = 11.7 | June 1, 2014
Small Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | < 65,000 Btu/h | AC | All | EER = 12.1 | October 29, 2003
≥ 65,000 Btu/h and < 135,000 Btu/h | AC | N-E A-O | EER = 12.1 EER = 11.9 | June 1, 2013
Large Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC AC | N-E A-O | EER = 12.0 EER = 11.8 | June 1, 2014
Very Large Commercial Package Air-Conditioning and Heating Equipment (Evaporatively-Cooled) | ≥ 240,000 Btu/h and < 760,000 Btu/h | AC AC | N-E A-O | EER = 11.9 EER = 11.7 | June 1, 2014
Small Commercial Package Air Conditioning and Heating Equipment (Water-Source: Water-to-Air, Water-Loop) | < 17,000 Btu/h ≥ 17,000 Btu/h and < 135,00 Btu/h | HP | All | EER = 12.2 | October 9, 2015
COP = 4.3 EER = 13.0 COP = 4.3
1 And manufactured before January 1, 2018. 2 And manufactured before January 1, 2023. 3 COP standard remains in effect on and after January 1, 2023. * E-N = Electric Resistance Heating or No Heating A-O = All Other Types of Heating
|  |  |  |  |  |  |  |  |

####

#### Table C-7
Standards for Single Package Vertical Air Conditioners and Single Package Vertical Heat Pumps Manufactured on or After January 1, 2010

Equipment Type | Cooling Capacity | Sub-category | Efficiency Levels | Compliance date: Products manufactured on and after
Single Package Vertical Air-Conditioners and Single Package Vertical Heat Pumps, single-phase and three-phase | < 65,000 Btu/h | AC | EER = 9.0 | January 1, 2010
EER = 11.0 | September 23, 2019
HP | EER = 9.0 COP = 3.0 | January 1, 2010
EER = 11.0 COP = 3.3 | September 23, 2019
Single Package Vertical Air-Conditioners and Single Package Vertical Heat Pumps | ≥ 65,000 Btu/h and < 135,000 Btu/h | AC | EER = 10.0 | October 9, 2015
HP | EER = 10.0 COP = 3.0
≥ 135,000 Btu/h and < 240,000 Btu/h | AC | EER = 10.0 | October 9, 2016
HP | EER = 10.0 COP = 3.0

#### Table C-8
Standards for Computer Room Air Conditioners

Equipment type | Net sensible ‘cooling capacity (Btu/hr) | Minimum SCOP ‘efficiency | Compliance date:
Downflow unit | Upflow unit
Air‐Cooled | <65,000 | 2.20 | 2.09 | October 29, 2012
≥65,000 and <240,000 | 2.10 | 1.99 | October 29, 2013
≥240,000 and <760,000 | 1.90 | 1.79 | October 29, 2013
Water‐Cooled | <65,000 | 2.60 | 2.49 | October 29, 2012
≥65,000 and <240,000 | 2.50 | 2.39 | October 29, 2013
≥240,000 and <760,000 | 2.40 | 2.29 | October 29, 2013
Water‐Cooled with a Fluid Economizer | <65,000 | 2.55 | 2.44 | October 29, 2012
≥65,000 and <240,000 | 2.45 | 2.34 | October 29, 2013
≥240,000 and <760,000 | 2.35 | 2.24 | October 29, 2013
Glycol‐Cooled | <65,000 | 2.50 | 2.39 | October 29, 2012
≥65,000 and <240,000 | 2.15 | 2.04 | October 29, 2013
≥240,000 and <760,000 | 2.10 | 1.99 | October 29, 2013
Glycol‐Cooled with a Fluid Economizer | <65,000 | 2.45 | 2.34 | October 29, 2012
≥65,000 and <240,000 | 2.10 | 1.99 | October 29, 2013
≥240,000 and <760,000 | 2.05 | 1.94 | October 29, 2013

#### Table C-9
Standards for Variable Refrigerant Flow Multi-Split Air Conditioners and Heat Pumps

Equipment type | Cooling capacity (Btu/h) | Heating type1 | ‘Efficiency level | Compliance date: Products manufactured on and after… |
VRF Multi-Split ‘Air Conditioners (Air-Cooled) | <65,000 | All | 13.0 SEER | June 16, 2008 |
≥65,000 and < 135,000 | N-E | 11.2 EER | January 1, 2010 |
A-O | 11.0 EER | January 1, 2010 |
≥135,000 and <240,000 | N-E | 11.0 EER | January 1, 2010 |
A-O | 10.8 EER | January 1, 2010 |
≥240,000 and <760,000 | N-E | 10.0 EER | January 1, 2010 |
A-O | 9.8 EER | January 1, 2010 |
VRF Multi-Split ‘Heat Pumps (Air-Cooled) | <65,000 | All | 13.0 SEER 7.7 HSPF | June 16, 2008 |
≥65,000 and < 135,000 | N-E | 11.0 EER 3.3 COP | January 1, 2010 |
A-O | 10.8 EER 3.3 COP | January 1, 2010 |
≥135,000 and <240,000 | N-E | 10.6 EER 3.2 COP | January 1, 2010 |
A-O | 10.4 EER 3.2 COP | January 1, 2010 |
≥240,000 Btu/h and <760,000 Btu/h | N-E | 9.5 EER 3.2 COP | January 1, 2010 |
A-O | 9.3 EER 3.3 COP | January 1, 2010 |
VRF Multi-Split Heat Pumps (Water Source) | <17,000 Btu/h | Without Heat Recovery | 12.0 EER 4.2 COP | October 29, 2012 October 29, 2003 |
With Heat Recovery | 11.8 EER 4.2 COP | October 29, 2012 October 29, 2003 |
≥17,000 Btu/h and <65,000 Btu/h | All | 12.0 EER 4.2 COP | October 29, 2003 |
≥65,000 Btu/h and <135,000 Btu/h | All | 12.0 EER 4.2 COP | October 29, 2003 |
≥135,000 Btu/h and <760,000 Btu/h | Without Heat Recovery | 10.0 EER 3.9 COP | October 29, 2013 |
With Heat Recovery | 9.8 EER 3.9 COP | October 29, 2013 |
1VRF Multi-Split Heat Pumps ( Air-Cooled ) with heat recovery fall under the category of “All Other Types of Heating” unless they also have electric resistance heating, in which case it falls under the category for “No Heating or Electric Resistance Heating.” *N-E = No Heating or Electric resistance heating A-O = All Other Types of Heating

#### Table C-10
Standards for Double-Duct Commercial Packaged Air Conditioning and Heating Equipment
Manufactured on or After January 1, 2010

Equipment Type | Cooling Capacity | Sub-category | Heating Type* | Efficiency Levels
Small Double-Duct Commercial Packaged Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 65,000 Btu/h and < 135,000 Btu/h | AC | E-N | EER = 11.2
A-O | EER = 11.0
HP | E-N | EER = 11.0 COP = 3.3
A-O | EER = 10.8 COP = 3.3
Large Commercial Double-Duct Packaged Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 135,000 Btu/h and < 240,000 Btu/h | AC | E-N | EER = 11.0
A-O | EER = 10.8
HP | E-N | EER = 10.6 COP = 3.2
A-O | EER = 10.4 COP = 3.2
Very Large Double-Duct Commercial Packaged Air-Conditioning and Heating Equipment (Air-Cooled) | ≥ 240,000 Btu/h and < 300,000 Btu/h | AC | E-N | EER = 10.0
A-O | EER = 9.8
HP | E-N | EER = 9.5 COP = 3.2
A-O | EER = 9.3 COP = 3.2
* E-N = No Heating or Electric Resistance Heating A-O = All Other Types of Heating 1For units tested using the relevant AHRI Standards, all COP values must be rated at 47◦F outdoor dry-bulb temperature for air-cooled equipment.

#### Table C-11
Standards for Direct Expansion-Dedicated Outdoor Air Systems Manufactured on or After May 1, 2024

Subcategory | Minimum Efficiency Level
(AC) -- Air-cooled without ventilation energy recovery systems | ISMRE2 = 3.8
(AC w/VERS) -- Air-cooled with ventilation energy recovery systems | ISMRE2 = 5.0
(ASHP) -- Air-source heat pumps without ventilation energy recovery systems | ISMRE2 = 3.8 ISCOP2 = 2.05
(ASHP w/VERS) -- Air-source heat pumps with ventilation energy recovery systems | ISMRE2 = 5.0 ISCOP2 = 3.20
(WC) -- Water-cooled without ventilation energy recovery systems | ISMRE2 = 4.7
(WC w/VERS) -- Water-cooled with ventilation energy recovery systems | ISMRE2 = 5.1
(WSHP) -- Water-source heat pumps without ventilation energy recovery systems | ISMRE2 = 3.8 ISCOP2 = 2.13
(WSHP w/VERS) -- Water-source heat pumps with ventilation energy recovery systems | ISMRE2 = 4.6 ISCOP2 = 4.04

(2) ‘Gas-fired ‘Air Conditioners and Heat Pumps. There is no energy efficiency standard or energy design standard for gas-fired air conditioners or gas-fired heat pumps.

(3) Other ‘Central Air Conditioners. See section 1605.3(c) of this Article for energy efficiency standards for other central air conditioners.

(4) ‘Heat Pump Water-Heating Packages. There is no energy efficiency standard or energy design standard for heat pump water-heating packages.

(5) ‘Air Filters. There are no energy efficiency standards or energy design standards for air filters.

### (d) Portable Air Conditioners, Evaporative Coolers, Ceiling Fans, Ceiling Fan Light Kits, Whole House Fans, Residential Exhaust Fans, Dehumidifiers, Residential Furnace Fans, and Commercial and Industrial Fans and Blowers.

(1) ‘Ceiling fans.

(A) All ceiling fans manufactured on or after January 1, 2007, shall have the following features:

1. Fan speed controls separate from any lighting controls;

2. Adjustable speed controls (either more than 1 speed or variable speed);

3. The capability of reversible fan action, except for:

a. Fans sold for industrial applications;

b. Fans sold for outdoor applications; and

c. Cases in which safety standards would be violated by the use of the reversible mode.

(B) Ceiling fans manufactured on or after January 21, 2020 shall meet the requirements shown in Table D-4.

#### Table D-4
Standards for Ceiling Fans Manufactured On or After January 21, 2020

Ceiling Fan Type | Minimum Efficiency (CFM/Watts)1
Very small-diameter (VSD) | D ≤ 12 inches: 21 D >12 inches: 3.16D – 17.04
Standard | 0.65 D + 38.03
Hugger | 0.29 D + 34.46
High-speed small-diameter (HSSD) | 4.16 D + 0.02
1D is the ceiling fan’s blade span, in inches.

(C) Large-Diameter Ceiling Fans. Large-diameter ceiling fans manufactured on or after

January 21, 2020, shall have a CFEI greater than or equal to:

1. 1.00 at high speed; and

2. 1.31 at 40 percent speed or the nearest speed that is not less than 40 percent speed.

EXCEPTIONS to Section 1605.1(d)(1) of this Article: The provisions in section 1605.1(d)(1) of this Article apply to ceiling fans except:

(1) Ceiling fans where the plane of rotation of a ceiling fan's blades is not less than or equal to 45 degrees from horizontal, or cannot be adjusted based on the manufacturer's specifications to be less than or equal to 45 degrees from horizontal;

(2) Centrifugal ceiling fans, as defined in section 1602(d) of this Article;

(3) Belt-driven ceiling fans, as defined in section 1602(d) of this Article;

(4) Oscillating ceiling fans, as defined in section 1602(d) of this Article; and

(5) Highly decorative ceiling fans, as defined in section 1602(d) of this Article.

(2) ‘Ceiling fan light kits.

(A) Ceiling Fan Light Kits with Medium Screw Base Sockets. Ceiling fan light kits manufactured on or after January 1, 2007, and prior to January 21, 2020, with medium screw base sockets must be packaged with medium screw base lamps to fill all sockets. These medium screw base lamps must:

1. Be compact fluorescent lamps that meet or exceed the requirements shown in Table D-5 or be as described in section 1605.1(d)(2)(A)2 of this Article:

#### Table D-5
Requirements for CFLs Used in Ceiling Fan Light Kits
with Medium Screw Base Sockets

Factor | Requirements
Rated Wattage (Watts) & Configuration1 | Minimum Initial Lamp Efficacy (lumens per Watt)2
Bare Lamp
Lamp Power < 15 | 45.0
Lamp Power ≥ 15 | 60.0
Covered Lamp (no reflector):
Lamp Power < 15 | 40.0
15 ≤ Lamp Power < 19 | 48.0
19 ≤ Lamp Power < 25 | 50.0
Lamp Power ≥ 25 | 55.0
With Relector:
Lamp Power < 20 | 33.0
Lamp Power ≥ 20 | 40.0
Lumen Maintenance at 1,000 hours | ≥ 90.0%
Lumen Maintenance at 40 percent of Lifetime | ≥ 80.0%
Rapid Cycle Stress Test | Each lamp must be cycled once for every 2 hours of lifetime. At least 5 lamps must meet or exceed the minimum number of cycles
Lifetime | ≥ 6,000 hours for the sample of lamps.
1Use rated wattage to determine the appropriate minimum efficacy requirements in this table. 2Calculate efficacy using measured wattage, rather than rated wattage, and measured lumens to determine product compliance. Wattage and lumen values indicated on products or packaging may not be used in calculation.

2. Be light sources other than compact fluorescent lamps that have lumens per watt performance at least equivalent to comparably configured compact fluorescent lamps meeting the energy conservation standards in section 1605.1(d)(1) of this Article.

(B) Ceiling Fan Light Kits with Pin-Based Sockets for Fluorescent Lamps. Ceiling fan light kits manufactured on or after January 1, 2007, and prior to January 21, 2020, with pin-based sockets for fluorescent lamps must use an electronic ballast and be packaged with lamps to fill all sockets. These lamp ballast platforms must meet the requirements shown in Table D-6:

#### Table D-6
System Efficacy Per Lamp Ballast Platform in Lumens Per Watt (lm/W)

Lamp Description | Minimum Lumens Per Watt (lm/W)
All lamps below 30 total listed lamp watts | 50 lm/w
All lamps that are ≤ 24 inches and ≥ 30 total listed lamp watts. | 60 lm/w
All lamps that are > 24 inches and ≥ 30 total listed lamp watts. | 70 lm/w

(C) Ceiling fan light kits manufactured on or after January 1, 2009, and prior to January 21, 2020. Ceiling fan light kits manufactured on or after January 1, 2009, and prior to January 21, 2020, with socket types other than those covered in sections 1605.1(d)(2)(A) and 1605.1(d)(2)(B) of this Article, including candelabra screw base sockets, must be packaged with lamps to fill all sockets and must not be capable of operating with lamps that total more than 190 watts.

(D) Ceiling fan light kits manufactured on or after January 21, 2020. Ceiling fan light kits manufactured on or after January 21, 2020 must be packaged with lamps to fill all sockets, and each basic model of lamp packaged with the basic model of the ceiling fan light kit and each basic model of integrated SSL in the ceiling fan light kit basic model shall meet the requirements shown in Table D-7:

#### Table D-7
Standards for Ceiling Fan Light Kits Manufactured On or After January 21, 2020

Lumens1 | Minimum required efficacy (lm/W)
< 120 | 50
≥ 120 | (74.0-29.42 x 0.9983lumens)
1Use the lumen output for each basic model of lamp packaged with the basic model of ceiling fan light kit (CFLK) or each basic model of integrated SSL in the CFLK basic model to determine the applicable standard.

1. Ceiling Fan Light Kits with Medium Screw Base Sockets. Ceiling fan light kits with medium screw base sockets manufactured on or after January 21, 2020 and packaged with compact fluorescent lamps must include lamps that also meet the requirements shown in Table D-8:

#### Table D-8
Standards for Ceiling Fan Light Kits with Medium Screw Base Sockets
Manufactured On or After January 21, 2020

Criteria | Requirement
Lumen Maintenance at 1,000 Hours | ≥ 90%‘
Lumen Maintenance at 40% of Lifetime | ≥ 80%
Rapid Cycle Stress Test | Each lamp must be cycled once for every 2 hours of lifetime of compact fluorescent lamp. At least 5 Lamps must meet or exceed the minimum number of cycles.
Lifetime | ≥ 6,000 hours for the sample of lamps

2. Ceiling Fan Light Kits with Pin Based Sockets for Fluorescent Lamps. Ceiling fan light kits with pin based sockets for fluorescent lamps, manufactured on or after January 21, 2020, must also use an electronic ballast

(3) Dehumidifiers.

(A) Dehumidifiers Manufactured On or After October 1, 2012 and Before June 13, 2019. The energy factor for dehumidifiers manufactured on or after October 1, 2012 and before June 13, 2019 shall be not less than the applicable values shown in Table D-9.

#### Table D-9
Standards for Dehumidifiers Manufactured
On or After October 1, 2012 And Before June 13, 2019

Product capacity (pint/day) | Minimum energy factor (liters/kWh)
Effective October 1, 2012
25.00 or less | 1.35
25.01 – 35.00 | 1.35
35.01 – 45.00 | 1.50
45.01 – 54.00 | 1.60
54.01 – 74.99 | 1.70
75.00 or more | 2.50

(B) Dehumidifiers Manufactured On or After June 13, 2019. The integrated energy factor for dehumidifiers manufactured on or after June 13, 2019 shall be not less than the applicable values shown in Table D-10.

#### Table D-10
Standards for Dehumidifiers Manufactured On or After June 13, 2019

Portable dehumidifier product capacity (pints/day) | Minimum Integrated Energy Factor (liters/kWh)
25.00 or less | 1.30
25.01 – 50.00 | 1.60
50.01 or more | 2.80
Whole-home dehumidifier product case volume (ft3)
8.0 or less | 1.77
More than 8.0 | 2.41

(4) Residential furnace fans. Residential furnace fans incorporated in the products listed in Table D-11 of this Article and manufactured on and after July 3, 2019, shall have a fan energy rating (FER) value that meets or is less than the values shown in Table D-11.

(A) Exceptions. Furnace fans incorporated into hydronic air handlers, SDHV modular blowers, SDHV electric furnaces, and central air conditioner/central heat pump indoor units are not subject to the standards listed in Table D-11.

#### Table D-11
Energy Conservation Standards for Federally Covered Residential Furnace Fans

Product Class | FER1 (Watts/1000cfm)
Non-Weatherized, Non-Condensing Gas Furnace Fan (NWG-NC) | FER = 0.044 x QMax + 182
Non-Weatherized, Condensing Gas Furnace Fan (NWG-C) | FER = 0.044 x QMax + 195
Weatherized, Non-Condensing Gas Furnace Fan (WG-NC) | FER = 0.044 x QMax + 199
Non-Weatherized, Non-Condensing Oil Furnace Fan (NWO-NC) | FER = 0.071 x QMax + 382
Non-Weatherized, Electric Furnace/Modular Blower Fan (NWEF/NWMB) | FER = 0.044 x QMax + 165
Mobile Home Non-Weatherized, Non-Condensing Gas Furnace Fan (MH-NWG-NC) | FER = 0.071 x QMax + 222
Mobile Home Non-Weatherized, Condensing Gas Furnace Fan (MH-NWG-C) | FER = 0.071 x QMax + 240
Mobile Home Electric Furnace/Modular Blower Fan (MH-EF/MB) | FER = 0.044 x QMax + 101
Mobile Home Non-Weatherized, Oil Furnace Fan (mh-nwo) | Reserved
Mobile Home Weatherized, Gas Furnace Fan (MH-WG)** | Reserved
1QMax is the airflow, in cfm, at the maximum airflow-control setting measured using the final DOE teat procedure at 10 CFR part 430, subpart B, appendix AA

(5) Portable Air Conditioners.

(A) Federally Regulated Portable Air Conditioners. Single-duct and dual-duct federally

regulated portable air conditioners manufactured on or after January 10, 2025, must

have a combined energy efficiency ratio (CEER) in Btu/Wh no less than SACC: Seasonally

adjusted cooling capacity in Btu/h, as determined in accordance with the test procedure

in section 1604(d) of this Article.

(B) State-Regulated Portable Air Conditioners. See section 1605.3(d) of this Article for

energy efficiency standards for state-regulated portable air conditioners manufactured

on or after February 1, 2020, but before January 10, 2025.

(6) There are no energy efficiency standards or energy design standards for spot air conditioners, evaporative coolers, whole house fans, or residential exhaust fans, or commercial and industrial fans and blowers.

### (e) Space Heating Products.

(1) Gas Vented Home Heating Equipment. The AFUE of gas vented home heating equipment manufactured on or after the effective dates shown shall be not less than the applicable values shown in Table E‐2.

#### Table E-2
Standards for Gas Vented Home Heating Equipment Manufactured on or After April 16, 2013

Product Class | Design Type | Capacity (Btu per hour) | Minimum AFUE (%)
Wall | Fan | ≤ 42,000 | 75
Wall | Fan | > 42,000 | 76
Wall | Gravity | ≤ 27,000 | 65
Wall | Gravity | > 27,000 and ≤ 46,000 | 66
Wall | Gravity | > 46,000 | 67
Floor | All | ≤ 37,000 | 57
Floor | All | > 37,000 | 58
Room | All | ≤ 20,000 | 61
Room | All | > 20,000 and ≤ 27,000 | 66
Room | All | > 27,000 and ≤ 46,000 | 67
Room | All | > 46,000 | 68

(2) Central Furnaces and Boilers. Central furnaces and boilers manufactured on or after the

effective dates shown shall meet all applicable requirements shown in Tables E-3, E-4, E-5,

and E-6.

#### Table E-3
Standards for Residential Boilers < 300,000 Btu/hour Input and Electric Residential Boilers

Appliance | Minimum AFUE (%) | Maximum Power Consumption
Effective September 1, 2012 | Effective January 15, 2021
AFUE | Standby | Off Mode
Gas steam boilers with single phase electrical supply | 801 | 821 | 8 | 8
Gas hot ‘water boilers with single phase electrical supply | 821, 2 | 841, 2 | 9 | 9
Oil steam ‘boilers with single phase electrical supply | 82 | 85 | 11 | 11
Oil hot water boilers with single phase electrical supply | 842 | 862 | 11 | 11
Electric steam residential boilers | NONE | NONE | 8 | 8
Electric hot water residential boilers | NONE2 | NONE2 | 8 | 8
¹ No constant burning pilot light design standard effective September 1, 2012. ² Automatic means for adjusting temperature design standard effective September 1, 2012. (Boilers equipped with tankless domestic water heating coils do not need to comply with this requirement.)
|  |  |  |  |  |  |

(A) Automatic Means for Adjusting Water Temperature. The automatic means for adjusting the temperature design, shown as footnote 2 in Table E‐3 immediately above, means:

1. In General. The manufacturer shall equip each gas, oil, and electric hot water boiler (other than a boiler equipped with a tankless domestic water heating coil) with automatic means for adjusting the temperature of the water supplied by the boiler to ensure that an incremental change in inferred heat load produces a corresponding incremental change in the temperature of water supplied.

2. Single ‘Input Rate. For a boiler that fires at one input rate, the requirements of this subparagraph may be satisfied by providing an automatic means that allows the burner or heating element to fire only when the means has determined that the inferred heat load cannot be met by the residual heat of the water in the system.

3. No Inferred Heat Load. When there is no inferred heat load with respect to a hot water boiler, the automatic means described in subsections 1605.1(e)(2)(A)1. and 1605.1(e)(2)(A)2. of this Article. shall limit the temperature of the water in the boiler to not more than 140°F.

4. Operation. A boiler described in subsections 1605.1(e)(2)(A)1. and 1605.1(e)(2)(A)2. of this Article. shall be operable only when the automatic means described in clauses subsections 1605.1(e)(2)(A)1. and 1605.1(e)(2)(A)2., 1605.1(e)(2)(A)3 of this Article is installed.

(B) EXCEPTION to Section 1605.1(e)(2) of this Article: A boiler that is manufactured to operate without any need for electricity or any electric connection, electric gauges, electric pumps, electric wires, or electric devices shall not be required to meet the efficiency standards or design standard that take effect for models manufactured on or after September 1, 2012. Boilers described in this EXCEPTION are required to meet the efficiency standards in effect prior to September 1, 2012, as applicable.

#### Table E-4
Standards for Gas- and Oil-Fired Commercial Packaged Boilers ≥ 300,000 Btu/hour Input

Appliance | Type | Rated Input (Btu/hr) | Minimum ‘Efficiency (%)
Combustion Efficiency % | Thermal Efficiency%
March 2, 2012 | March 2, 2012 through March 1, 2022 | March 2, 2022
Hot Water Boilers | ‘Gas‐fired | ≥ 300,000 and ≤2,500,000 |  | 80 | 80
> 2,500,000 | 82 | — | —
Oil‐fired | ≥ 300,000 and ≤2,500,000 |  | 82 | 82
> 2,500,000 | 84 | — | —
Steam ‘Boilers | Gas‐fired, except natural draft | ≥ 300,000 and ≤2,500,000 |  | 79 | 79
> 2,500,000
Gas‐fired, natural draft | ≥ 300,000 and ≤2,500,000 |  | 77 | 79
> 2,500,000
Oil‐fired | ≥ 300,000 and ≤2,500,000 |  | 81 | 81
> 2,500,000

#### Table E-5
Standards for Commercial Central Warm Air Furnaces

Appliance | Rated Input (Btu/hr) | Minimum Thermal Efficiency
January 1, 1994 | January 1, 2023
Gas central warm air furnaces | ≥ 225,000 | 80 | 81
Oil central warm air furnaces | ≥ 225,000 | 81 | 82

#### Table E-6
Standards for Residential Central Furnaces

Product class | AFUE (percent) | Maximum Electrical Power Consumption
Standby | Off Mode
(A) Non-weatherized ‘gas furnaces (not including mobile home furnaces) | 80 | No requirement
(B) Mobile Home gas furnaces | 80 | No requirement
(C) Non-weatherized oil-fired furnaces (not including mobile home furnaces) | 83 | 11 | 11
(D) Mobile Home oil-fired furnaces | 75 | 11 | 11
(E) Weatherized gas furnaces | 81 | No requirement
(F) Weatherized oil-fired furnaces | 78 | No requirement
(G) Electrical furnaces | 78 | 10 | 10

(3) Unit Heaters. Unit heaters manufactured on or after August 8, 2008 shall:

(A) Be equipped with an intermittent ignition device; and

(B) Have power venting or an automatic flue damper. An automatic vent damper is an acceptable alternative to an automatic flue damper for those unit heaters where combustion air is drawn from the conditioned space.

(4) Duct Furnaces. See section 1605.3(e) of this Article for energy efficiency and energy design standards for duct furnaces.

(5) Combination Space-Heating and Water-Heating Appliances. See Section 1605.3(e)of this Article for requirements for combination space-heating and water-heating appliances.

(6) There are no energy efficiency standards or energy design standards for infrared gas space

(7) heaters.

### (f) Water Heaters.

(1) Water Heaters Regulated Under 10 C.F.R. section 430.32(d). The uniform energy factor of water heaters regulated under 10 C.F.R. section 430.32(d) shall be not less than the applicable values shown in Table F-2.

#### Table F-2
Standards for Water Heaters Regulated Under 10 C.F.R. Section 430.32(d)

Product Class | Rated Storage Volume and Input Rating (if applicable) | Draw Pattern | Minimum Uniform Energy Factor*
Gas-Fired Storage Water Heater | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.3456 – (0.0020 x Vr)
Low | 0.5982 – (0.0019 x Vr)
Medium | 0.6483 – (0.0017 x Vr)
High | 0.6920 – (0.0013 x Vr)
> 55 gallons and ≤ 100 gallons | Very small | 0.6470 – (0.0006 x Vr)
Low | 0.7689 – (0.0005 x Vr)
Medium | 0.7897 – (0.0004 x Vr)
High | 0.8072 – (0.0003 x Vr)
Oil-Fired Storage Water Heater | ≤ 50 gallons | Very small | 0.2509 – (0.0012 x Vr)
Low | 0.5330 – (0.0016 x Vr)
Medium | 0.6078 – (0.0016 x Vr)
High | 0.6815 – (0.0014 x Vr)
Electric Storage Water Heaters | ≥ 20 gallons and ≤ 55 gallons | Very small | 0.8808 – (0.0008 x Vr)
Low | 0.9254 – (0.0003 x Vr)
Medium | 0.9307 – (0.0002 x Vr)
High | 0.9349 – (0.0001 x Vr)
> 55 gallons and ≤ 120 gallons | Very small | 1.9236 – (0.0011 x Vr)
Low | 2.0440 – (0.0011 x Vr)
Medium | 2.1171 – (0.0011 x Vr)
High | 2.2418 – (0.0011 x Vr)
Tabletop Water Heater | ≥ 20 gallons and ≤ 120 gallons | Very small | 0.6323 – (0.0058 x Vr)
Low | 0.9188 – (0.0031 x Vr)
Medium | 0.9577 – (0.0023 x Vr)
High | 0.9884 – (0.0016 x Vr)
Instantaneous Gas-fired Water Heater | < 2 gallons and > 50,000 Btu/h | Very small | 0.80
Low | 0.81
Medium | 0.81
High | 0.81
Instantaneous Electric Water Heater | < 2 gallons | Very small | 0.91
Low | 0.91
Medium | 0.91
High | 0.92
Grid-Enabled Water Heater | > 75 gallons | Very small | 1.0136 – (0.0028 x Vr)
Low | 0.9984 – (0.0014 x Vr)
Medium | 0.9853 – (0.0010 x Vr)
High | 0.9720 – (0.0007 x Vr)
*Vr = Rated Storage Volume in gallons

(2) Water Heaters Regulated Under 42 U.S.C. section 6295(e)(1). Water heaters regulated under 42 U.S.C. section 6295(e)(1) must meet the values shown in Table F-3 as applicable.

#### Table F-3
Standards for Water Heaters Regulated Under 42 U.S.C. section 6295(e)(1)

Product Class | Minimum Energy Factor*
Gas Water Heater1 | 0.62 – (0.0019 x Vr)
Oil Water Heater1 | 0.59 – (0.0019 x Vr)
Electric Water Heater1 | 0.95 – (0.00132 x Vr)
*Vr = Rated Storage Volume in gallons 1Applies to water heaters not covered under 10 C. F.R. section 430.32, including but not limited to storage water heaters >1 gal and < 20 gal (mini-tank water heaters) and booster water heaters. These standards will take effect on the effective date of a federal test procedure that converts Uniform Energy Factor (UEF) to Energy Factor for these products. If the Secretary adopts federal efficiency standards for water heaters regulated under 42 U. S. C. section 6295(e)(1), these standards shall not apply

(3) Water Heaters Regulated Under 10 C.F.R. section 431.110. Water heaters regulated under 10 C.F.R. section 431.110 must meet the values shown in Tables F-4 and F-5, as applicable.

(A) Commercial Storage Water Heaters, Instantaneous Water Heaters, and Hot Water Supply Boilers (Excluding Residential-Duty Commercial Water Heaters). Each commercial storage water heater, instantaneous water heater, and hot water supply boiler (excluding residential-duty commercial water heaters) must meet the applicable energy conservation standard level(s) as specified in Table F-4.

1. Packaged Boiler Exclusion. Any packaged boiler that provides service water that meets the definition of “commercial packaged boiler” in section 1602(e) of this Article, but does not meet the definition of “hot water supply boiler” in section 1602(f) of this Article, must meet the requirements that apply to it under section 1605.1(e) of this Article.

#### Table F-4
Standards for Water Heaters Regulated Under 10 C.F.R. Section 431.110(a)
(Excluding Residential-Duty Commercial Water Heaters)

Equipment Category | Size | Energy Conservation Standardsa
Maximum standby lossc (equipment manufactured on and after October 29, 2003)b | Minimum thermal efficiency (equipment manufactured on and after October 9, 2015)b (%)
Electric storage water heaters | All | 0.30 + 27/Vm (%/hr) | N/A
Gas-fired storage water heaters | ≤ 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
> 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Oil-fired storage water heaters | ≤ 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
> 155,000 Btu/hr | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Gas-fired instantaneous water heaters and hot water supply boilers | < 10 gallons | N/A | 80
≥ 10 gallons | Q/800 + 110(Vr) ½ (Btu/hr) | 80
Oil-fired instantaneous water heaters and hot water supply boilers | < 10 gallons | N/A | 80
≥ 10 gallons | Q/800 + 110(Vr) ½ (Btu/hr) | 78
aVm is the measured storage volume (in gallons), and Vr is the rated volume (in gallons). Q is the nameplate input rate in Btu/hr. bFor hot water supply boilers with a capacity of less than 10 gallons: (1) The standards are mandatory for products manufactured on and after October 21, 2005; and (2) products manufactured prior to that date, and on or after October 23, 2003, must meet either the standards listed in Table F-4 or the applicable standards in section 1605.1(e) of this Article for a “commercial packaged boiler.” cWater heaters and hot water supply boilers having more than 140 gallons of storage capacity need not meet the standby loss requirement if: (1) The tank surface area is thermally insulated to R-12.5 or more (2) a standing pilot light is not used; and (3) for gas or oil-fired storage water heaters, they have a fire damper or fan-assisted combustion.

(B) Residential-Duty Commercial Water Heaters. Each residential-duty commercial water heater must have a minimum uniform energy factor not less than the values shown in Table F-5.

#### Table F-5
Standards for Residential-Duty Commercial Water Heaters

Product Class | Specifications | Draw Pattern | Minimum Uniform Energy Factor*
Gas-Fired Storage | >75 kBtu/hr and ≤ 105 kBtu/hr and ≤ 120 gallons | Very Small | 0.2674 – (0.0009 x Vr)
Low | 0.5362 – (0.0012 x Vr)
Medium | 0.6002 – (0.0011 x Vr)
High | 0.6597 – (0.0009 x Vr)
Oil-Fired Storage | > 105 kBtu/hr and ≤ 140 kBtu/hr and ≤ 120 gallons | Very Small | 0.2932 – (0.0015 x Vr)
Low | 0.5596 – (0.0018 x Vr)
Medium | 0.6194 – (0.0016 x Vr)
High | 0.6740 – (0.0013 x Vr)
Electric Instantaneous | >12 kW and ≤ 58.6 kW and ≤ 2 gallons | Very small | 0.80
Low | 0.80
Medium | 0.80
High | 0.80
aAdditionally, to be classified as a residential-duty commercial water heater, a commercial water heater must meet the following conditions: (1) if the water heater requires electricity, it must use a single-phase external power supply; and (2) the water heater must not be designed to heat water to temperatures greater than 1800F. bVr is the rated storage volume (in gallons), as determined pursuant to 10 CFR section 429.44

(4) Combination Space-Heating and Water-Heating Appliances. See section 1605.3(e) of this Article for standards for combination space-heating and water-heating appliances.

### (g) Pool Heaters; Portable Electric Spas; Residential Pool Pump and Motor Combinations, and Replacement Residential Pool Pump Motors; and Pumps, Dedicated-Purpose Pool Pumps, and Replacement Dedicated-Purpose Pool Pump Motors.

(1) ‘Energy Efficiency Standard for Fossil Fuel-Fired Pool Heaters. The thermal efficiency of fossil fuel-fired pool heaters manufactured on or after the effective dates shown shall be not less than the values shown in Table G-1.

#### Table G-1
Standards for Fossil Fuel-Fired Pool Heaters

Appliance | Effective Date | Minimum Thermal ‘Efficiency (%)
‘Gas-Fired ‘Pool Heaters | April 16, 2013 | 82
Oil-Fired Pool Heaters | January 1, 1990 | 78

(2) ‘Energy ‘Efficiency Standards for Heat Pump Pool Heaters. See Section 1605.3(g) of this Article for energy ‘efficiency standards for heat pump pool heaters.

(3) Energy Efficiency Standard for Electric Resistance Pool Heaters. There is no energy efficiency standard for electric resistance pool heaters.

(4) Energy Design Standards for Pool Heaters. See Section 1605.3(g) of this Article for energy design standards for pool heaters.

(5) Energy ‘Efficiency Standards for Portable Electric Spas. See Section 1605.3(g) of this Article for energy ‘efficiency standards for portable electric spas.

(6) Energy Efficiency Standards for Pumps

(A) For the purposes of section 1605.1(g)(6)(B) of this Article, “PEICL” means the constant load pump energy index and “PEIvL” means the variable load pump energy index, both as determined in accordance with the test procedure in section 1604(g)(3)(A) of this Article. For the purposes of section 1605.1(g)(6)(D) of this Article, “BEP” means the best efficiency point as determined in accordance with the test procedure in section section 1604(g)(3)(A) of this Article.

(B) Pump Efficiency Standards. Each pump that is manufactured on or after January 27, 2020 and that:

1. is in one of the equipment classes listed in Table G-2 in section 1605.1(g)(6)(B)4 of this Article;

2. meets the definition of a “clean water pump” in section 1602(g)(4). of this Article;

3. is not listed in section 1605.1(g)(6)(C) of this Article; and

4. conforms to the characteristics listed in section 1605.1(g)(6)(D) of this Article must have a PEICL or PEIvL rating of not more than 1.00 using the appropriate C-value in Table G-2:

#### Table G-2
Standards for Pumps Manufactured On or After January 27, 2020

Equipment Class1 | Maximum PEI2 | C-value3
ESCC.1800.CL | 1.00 | 128.47
ESCC.3600.CL | 1.00 | 130.42
ESCC.1800.VL | 1.00 | 128.47
ESCC.3600.VL | 1.00 | 130.42
ESFM.1800.CL | 1.00 | 128.85
ESFM.3600.CL | 1.00 | 130.99
ESFM.1800.VL | 1.00 | 128.85
ESFM.3600.VL | 1.00 | 130.99
IL.1800.CL | 1.00 | 129.30
IL.3600.CL | 1.00 | 133.84
IL.1800.VL | 1.00 | 129.30
IL.3600.VL | 1.00 | 133.84
RSV.1800.CL | 1.00 | 129.63
RSV.3600.CL | 1.00 | 133.20
RSV.1800.VL | 1.00 | 129.63
RSV.3600.VL | 1.00 | 133.20
ST.1800.CL | 1.00 | 138.78
ST.3600.CL | 1.00 | 134.85
ST.1800.VL | 1.00 | 138.78
ST.3600.VL | 1.00 | 134.85
1Equipment class designations consist of a combination (in sequential order separated by periods) of: (1) An equipment family (ESCC = end suction close-coupled, ESFM – end suction frame mounted/own bearing, IL = in-line, RSV = radially split, multi-stage, vertical, in-line diffuser casing, ST = submersible turbine; all as defined in 10 C.F.R. section 431.462); (2) nominal speed of rotation (1800 = 1800 rpm, 3600 = 3600 rpm); and (3) an operating mode (CL = constant load, VL = variable load). Determination of the operating mode is determined using the test procedure in appendix A to this subpart. 2For equipment classes ending in .CL, the relevant PEI is PEICL. For equipment classes ending in .VL, the relevant PEI is PEIVL. 3The C-values shown in this table must be used in the equation for PERSTD when calculating PEICL or PEIVL, as described in section II.B of 10 C.F.R. Appendix A to subpart Y of part 431.

(C) Exceptions to Pump Efficiency Standards. The energy efficiency standards in section 1605.1(g)(6)(B) of this Article do not apply to the following pumps:

1. fire pumps;

2. self-priming pumps;

3. prime-assist pumps;

4. magnet driven pumps;

5. pumps designed to be used in a nuclear facility subject to 10 C.F.R. part 50, “Domestic Licensing of Production and Utilization Facilities”;

6. pumps meeting the military specification design and construction requirements set forth in 10 C.F.R. section 431.465(c)(6).

(D) Characteristics of Regulated Pumps. The energy conservation standards in section 1605.1(g)(6)(B) of this Article apply only to pumps that have the following characteristics:

1. flow rate of 25 gpm or greater at BEP at full impeller diameter;

2. maximum head of 459 feet at BEP at full impeller diameter and the number of stages required for testing;

3. design temperature range from 14 to 248oF;

4. designed to operate with either:

a. a 2- or 4-pole induction motor; or

b. a non-induction motor with a speed of rotation operating range that includes speeds of rotation between 2,880 and 4,320 revolutions per minute and/or 1,440 and 2,160 revolutions per minute; and

c. in either case, the driver and impeller must rotate at the same speed;

5. for ST pumps, a 6-inch or smaller bowl diameter; and

6. for ESCC and ESFM pumps, specific speed less than or equal to 5,000 when calculated using U.S. customary units.

(7) Energy Efficiency Standards for Dedicated Purpose Pool Pumps

(A) For the purposes of 1605.1(g)(7)(B) of this Article, “WEF” means the weighted energy factor and “hhp” means the rated hydraulic horsepower, as determined in accordance with the test procedure in section 1604(g)(3)(B) of this Article and applicable sampling plans in 10 C.F.R. section 429.59.

(B) Each dedicated-purpose pool pump that is not a submersible pump and is manufactured on or after July 19, 2021, shall have a WEF rating that is not less than the value calculated from Table G-3 in section 1605.1(g)(7)(B) of this Article:

#### Table G-3: Standards for Dedicated-Purpose Pool Pumps Manufactured on or After July 19, 2021

Equipment Class |  |  | Minimum allowable WEF score [kgal/kWh]
Dedicated-purpose pool pump variety | hhp Applicability | Motor phase |
Self-priming pool filter pumps | 0.711 hp ≤ hhp < 2.5 hp | Single | WEF = 2.30 * ln (hhp) + 6.59.
Self-priming pool filter pumps | hhp <0.711 hp | Single | WEF = 5.55, for hhp ≤ 0.13 hp -1.30 * ln (hhp)+ 2.90, for hhp >0.13 hp.
Non-self-priming pool filter pumps | hhp <2.5 hp | Any | WEF = 4.60, for hhp ≤ 0.13 hp -0.85 * ln (hhp) + 2.87, for hhp >0.13 hp.
Pressure cleaner booster pumps | Any | Any | WEF = 0.42.

(C) Each integral cartridge-filter pool pump and integral sand-filter pool pump that is manufactured on or after July 19, 2021, shall be distributed in commerce with a pool pump timer that is either integral to the pump or a separate component that is shipped with the pump.

(D) For all dedicated-purpose pool pumps manufactured on or after July 19, 2021, with freeze protection controls, the pump shall be shipped with freeze protection disabled or with all of the following default, user-adjustable settings:

1. the default dry-bulb air temperature setting shall be no greater than 40oF;

2. the default run time setting shall be no greater than 1 hour (before the temperature is rechecked); and

3. the default motor speed shall not be more than one half of the maximum available speed.

(E) Waterfall pumps. There is no energy efficiency standard for waterfall pumps. See 1605.1(g)(7)(D) of this Article for energy design standards for waterfall pumps with freeze protection controls.

(8) Energy Efficiency Standards and Energy Design Standards for Residential Pool Pump and Motor Combinations, Replacement Dedicated-Purpose Pool Pump Motors, and Replacement Residential Pool Pump Motors. See section 1605.3(g) of this Article for energy efficiency standards and energy design standards for residential pool pump and motor combinations, replacement dedicated-purpose pool pump motors, and replacement residential pool pump motors.

### (h) Plumbing Fittings.

(1) Metering Faucets and Wash Fountains. The flow rate of wash fountains and metering faucets shall be not greater than the applicable values shown in Table H‐1.

#### Table H-1
Standards for Plumbing Fittings

Appliance | Maximum Flow Rate
Wash fountains | 2.2 x rim space (inches)/20 gpm at 60psi
Metering ‘faucets | 0.25 gallons/cycle 1, 2
Metering faucets for wash fountains | 0.25xrim space (inches)/20 gpm at 60 psi 1, 2
1Sprayheads with independently‐controlled orifices and manual controls. The maximum flow rate of each orifice that delivers a pre‐set volume of water before gradually shutting itself off shall not exceed the maximum flow rate for a metering faucet. 2Sprayheads with collectively‐controlled orifices and metered controls. The maximum flow rate of a sprayhead that delivers a pre‐set volume of water before gradually shutting itself off shall be the product of (a) the maximum flow rate for a metering ‘faucet and (b) the number of component lavatories (rim space of the lavatory in inches (millimeters) divided by 20 inches (508 millimeters)).

(2) Showerhead‐Tub Spout Diverter Combinations. ‘Showerhead‐tub spout diverter combinations shall meet both the standard for showerheads and the standard for tub spout diverters.

(3) Tub Spout Diverters. See Section 1605.3(h) for standards for tub spout diverters.

(4) Commercial Pre‐rinse Spray Valves.

(A) The flow rate of commercial pre-rinse spray valves manufactured on or after January 1, 2006 and before January 28, 2019 shall be equal to or less than 6 gpm at 60 psi.

(B) The flow rate of commercial pre-rinse spray valves manufactured on or after January 28, 2019 shall be equal to or less than the values shown in Table H-2.

#### Table H-2
Standards for Commercial Pre-rinse Spray Valves
Manufactured On or After January 28, 2019

Product Class (spray force in ounce force (ozf) | Maximum Flow Rate (gpm)
Product Class 1 ( ≤ 5.0 ozf) | 1.00
Product Class 2( > 5.0 ozf and ≤ 8.0 ozf) | 1.20
Product Class 3 ( > 8.0 ozf ) | 1.28

(C) See section 1605.3(h) of this Article for design standards for commercial pre-rinse spray valves.

(5) Showerheads, lavatory faucets, kitchen faucets, aerators, and public lavatory faucets. See Section 1605.3 (h) of this Article for standards for all showerheads, lavatory faucets, kitchen faucets, aerators, and public lavatory faucets sold or offered for sale in California.

### (i) Plumbing Fixtures.

See Section 1605.3(i) of this Article for water ‘efficiency standards for plumbing fixtures.

### (j) Fluorescent Lamp Ballasts and Deep-Dimming Flourescent Lamp Ballasts.

(1) Fluorescent lamp ballasts (other than dimming ballasts). Except as provided in sections 1605.1(j)(2) and 1605.1(j)(3) of this Article, each fluorescent lamp ballast:

(A) Manufactured on or after November 14, 2014;

(B) Designed and marketed:

1. To operate at nominal input voltages at or between 120 and 277 volts;

2. To operate with an input current frequency of 60 Hertz; and

3. For use in connection with fluorescent lamps (as defined in 10 C.F.R. part 430, section 430.2)

(C) Shall have:

1. A power factor of 0.9 or greater except for ballasts that are not residential ballasts;

2. A power factor of 0.5 or greater for residential ballasts;

3. A ballast luminous efficiency not less than the values shown in Table J-2:

#### Table J-2
Standards for Fluorescent Lamp Ballasts, Except for Certain Dimming Ballasts
Applicable to Models Described in Section 1605.1(j)(1) of this Article

BLE = A/(1 +B*average total lamp arc power ᴧ -C) Where A, B, and C are as follows:
Description | A | B | C
Instant start and rapid start ballasts (not classified as residential) that are designed to operate | 0.993 | 0.27 | 0.25
4‐foot medium bipin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
8-foot slimline lamps |  |  |
Programmed start ballasts (not classified as residential) that are designed to operate | 0.993 | 0.51 | 0.37
4‐foot medium bipin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
4‐foot miniature bipin standard output lamps |  |  |
4‐foot miniature bipin high output lamps |  |  |
Instant start and rapid start ballasts (not classified as sign ballasts) that are designed to operate 8-foot high output lamps | 0.993 | 0.38 | 0.25
Programmed start ballasts (not classified as sign ballasts) that are designed to operate 8-foot high output lamps | 0.973 | 0.70 | 0.37
Sign ballasts that operate 8-foot high output lamps | 0.993 | 0.47 | 0.25
Instant start and rapid start residential ballasts that operate | 0.993 | 0.41 | 0.25
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |
8-foot slimline lamps |  |  |
Programmed start residential ballasts that are designed to operate | 0.973 | 0.71 | 0.37
4‐foot medium bi‐pin lamps |  |  |
2‐foot U‐shaped lamps |  |  |

(2) Certain Dimming Ballasts. Except as provided in section 1605.1(j)(3) of this Article, each dimming ballast:

(A) Manufactured on or after November 14, 2014; designed and marketed to operate one F34T12, two F34T12, two F96T12/ES, or two F96T12HO/ES lamps; and

(B) Designed and marketed:

1. To operate at nominal input voltages of 120 or 277 volts;

2. To operate with an input current frequency of 60 Hertz; and

3. For use in connection with fluorescent lamps (as defined in 10 C.F.R. part 430, section 430.2);

(C) Must have a power factor of:

1. 0.9 or greater for ballasts that are not residential ballasts; or

2. 0.5 or greater for residential ballasts; and

(D) A ballast luminous efficiency not less than the values shown in Table J-3:

#### Table J-3
Standards for Certain Dimming Fluorescent Lamp Ballasts, Ballast Luminous Efficiency Applicable
to Models Described in section 1605.1(j)(1).
of this Article

Designed for the Operation of | Ballast Input Voltage | Total Nominal Lamp Watts | Ballast Luminous Efficiency
Low Frequency Ballasts | High Frequency Ballasts
One F34T12 lamp | 120 / 277 | 34 | 0.777 | 0.778
Two F34T12 lamps | 120 / 277 | 68 | 0.804 | 0.805
Two F96T12/ES lamps | 120 / 277 | 120 | 0.876 | 0.884
Two F96T12HO/ES lamps | 120 / 277 | 190 | 0.711 | 0.713

Exceptions to Sections 1605.1(j)(1) and 1605.1(j)(2) . of this Article. The power factor and ballast luminous efficiency standards described in sections 1605.1(j)(1) and 1605.1(j)(2) of this Article do not apply to:

(1) a dimming ballast designed and marketed to operate exclusively lamp types other than one F34T12, two F34T12, two F96T12/ES, or two F96T12HO/ES lamps;

(2) a low frequency ballast that is designed and marketed to operate T8 diameter lamps; is designed and marketed for use in electromagnetic-interference-sensitive-environments only; and is shipped by the manufacturer in packages containing 10 or fewer ballasts; or

(3) a programmed start ballast that operates 4-foot medium bipin T8 lamps and delivers on average less than 140 milliamperes to each lamp.

(3) Mercury Vapor Lamp Ballasts. ‘Mercury vapor lamp ballasts, other than specialty application mercury vapor lamp ballasts, shall not be manufactured or imported into the United States after January 1, 2008.

### (k) Lamps.

(1) Federally‐Regulated General Service Fluorescent Lamps.

Each of the following federally regulated general service fluorescent lamps manufactured on or after the effective dates shown shall meet or exceed the lamp efficacy standards shown in Table K-2

#### Table K-2
Standards for Federally-Regulated General Service Fluorescent Lamps
Manufactured On or After July 15, 2012

Appliance | Correlated Color Temperature | Minimum Average Lamp Efficacy (LPW)
Effective July 15, 2012 | Effective January 26, 2018
4‐foot medium bipin lamps | ≤ 4,500K | 89 | 92.4
> 4,500K and ≤ 7,000K | 88 | 88.7
2‐foot U‐shaped lamps | ≤ 4,500K | 84 | 85.0
> 4,500K and ≤ 7,000K | 81 | 83.3
8-foot slimline lamps | ≤ 4,500K | 97 | 97.0
> 4,500K and ≤ 7,000K | 93 | 93.0
8‐foot high output lamps | ≤ 4,500K | 92 | 92.0
> 4,500K and ≤ 7,000K | 88 | 88.0
4-foot miniature bipin standard output | ≤ 4,500K | 86 | 95.0
> 4,500K and ≤ 7,000K | 81 | 89.3
4-foot miniature bipin high output | ≤ 4,500K | 76 | 82.7
> 4,500K and ≤ 7,000K | 72 | 76.9

(2) General Service Lamps. See section 1605.3(k) of this Article for energy efficiency standards for general service lamps.

(3) State-Regulated LED Lamps. See section 1605.3(k) of this Article for energy efficiency and energy design standards for state-regulated LED lamps.

(4) State-Regulated Small Diameter Directional Lamps. See section 1605.3(k) of this Article for energy efficiency and energy design standards for state-regulated small diameter directional lamps.

(5) GU24 Base Lamps. See section 1605.3(k) of this Article for energy design standards for GU24 base lamps.

### (l) Emergency Lighting.

(1) Emergency Lighting. An illuminated exit sign manufactured on or after January 1, 2006 shall have an input power demand of five watts or less per face.

### (m) Traffic Signal Modules.

(1) Traffic Signals for Vehicle and Pedestrian Control. Federally regulated traffic signals for vehicle and pedestrian control manufactured on or after January 1, 2006 shall have a nominal wattage and maximum wattage no greater than the values shown in Table M‐1, and shall be installed with compatible electrically connected signal control interface devices and conflict monitoring systems.

#### Table M-1
Standards for Traffic Signals for Vehicle and Pedestrian Control

Appliance | Maximum Wattage (at 74°C) | Nominal Wattage (at 25°C)
Traffic Signal Module Type:
12‐inch; Red Ball | 17 | 11
8‐inch; Red Ball | 13 | 8
12‐inch; Red Arrow | 12 | 9
12‐inch; Green Ball | 15 | 15
8‐inch; Green Ball | 12 | 12
12‐inch; Green Arrow | 11 | 11
Pedestrian Module Type:
Combination Walking Man/Hand | 16 | 13
Walking Man | 12 | 9
Orange Hand | 16 | 13

(2) See Section 1605.3(m) of this Article for energy ‘efficiency standards for traffic signal modules for pedestrian control sold or offered for sale in California.

### (n) Luminaires and Torchieres.

(1) Torchieres. Torchieres manufactured on or after January 1, 2006 shall consume not more than 190 watts of ‘power and shall not be capable of operating with lamps that total more than 190 watts.

(2) Metal Halide Lamp Fixtures.

(A) See Section 1605.3(n) of this Article for energy efficiency standards and energy design standards for luminaires, including standards for metal halide luminaires sold or offered for sale in California that are manufactured on or after January 1, 2010.

(B) Each metal halide lamp fixture, designed to be operated with lamps less than 150 W and greater than 500 W, manufactured on or after February 10, 2017, must contain a metal halide ballast with an efficiency not less than the value determined from the appropriate equation shown in Table N-1.

#### Table N-1
Standards for Metal Halide Lamp Fixtures Manufactured On or After February 10, 2017

Designed to be operated with ‘lamps of the following rated ‘lamp wattage | Tested input voltage‡‡ | Minimum standard equation‡‡%
≥ 50W and ≤ 100W | Tested at 480 V | (1/(1+1.24xP^(-0.351)))-0.020†;
≥ 50W and ≤ 100W | All others | 1/(1+1.24xP^(-0.351))
> 100W and < 150†;W | Tested at 480 V | (1/(1+1.24xP^(-0.351)))-0.020†;
> 100W and < 150†;W | All others | 1/(1+1.24xP^(-0.351))
> 500W and ≤ 1000W | Tested at 480 V | For >500W and ≤ 750W: 0.900
For >750W and ≤ 1000W: 0.000104xP+0.822
For >500W and ≤ 1000W: may not utilize a probe-start ballast
> 500W and ≤ 1000W | All others | For >500W and ≤ 750W: 0.910
For >750W and ≤ 1000W: 0.000104xP+0.832
For >500W and ≤ 1000W: may not utilize a probe-start ballast
† Includes 150 W fixtures specified in 10 C.F.R. section 431.326 paragraph (b)(3), that are fixtures rated only for 150 W lamps; rated for use in wet locations, as specified by the NFPA 70 section 410.4(A); and containing a ballast that is rated to operate at ambient air temperatures above 500 C †† P is defined as the rated wattage of the lamp the fixture is designed to operate. ‡‡ Tested input voltage is specified in 10 C.F.R section 431.324.

(C) Metal halide lamp fixtures manufactured on or after February 10, 2017, that operate lamps with rated wattage >500 W to = 1000 W must not contain a probe-start metal halide ballast.

EXCEPTION to Sections 1605.1(n)(2)(B) and 1605.1(n)(2)(C). of this Article, The standards described in sections 1605.1(n)(2)(B) and 1605.1(n)(2)(C) of this Article do not apply to metal halide lamp fixtures:

(1) with regulated-lag ballasts;

(2) that use electronic ballasts that operate at 480 volts; and

(3) that use high-frequency electronic ballasts.

### (o) Dishwashers.

The maximum ‘energy use and maximum ‘water use of dishwashers that are consumer products manufactured on or after the effective dates shown shall meet the applicable values shown in Table O.

#### Table O
Standards for Dishwashers

Appliance | Effective May 30, 2013
Maximum ‘Energy Use (kWh/year) | Maximum ‘Water Use (gallons/cycle)
Compact ‘dishwashers | 222 | 3.5
Standard dishwashers | 307 | 5.0

### (p) Clothes Washers.

(1) Standards for Residential Clothes Washers. Clothes washers that are consumer products manufactured on or after the effective dates shown shall have an integrated modified energy factor not less than, and an integrated water factor not greater than the applicable values shown in Table P-1.

#### Table P-1
Standards for Residential Clothes Washers Manufactured On or After March 7, 2015

Appliance | Minimum Integrated Modified ‘Energy Factor | Maximum Integrated Water Factor
March 7, 2015 | January 1, 2018 | March 7, 2015 | January 1, 2018
Top‐loading, Compact | 0.86 | 1.15 | 14.4 | 12.0
Top‐loading, Standard | 1.29 | 1.57 | 8.4 | 6.5
Front‐loading, Compact | 1.13 | 1.13 | 8.3 | 8.3
Front‐loading, Standard | 1.84 | 1.84 | 4.7 | 4.7
|  |  |  |  |  |  |  |

(2) Commercial Clothes Washers. Commercial clothes washers manufactured on or after the effective dates shown shall have a modified energy factor not less than, and a water factor not greater than, the applicable values shown in Table P-2.

#### Table P-2
Standards for Commercial Clothes Washers

Appliance | Minimum Modified Energy Factor | Maximum Water Factor
Effective January 8, 2013 | Effective January 8, 2013
Top-loading clothes washers | 1.60 | 8.5
Front-loading clothes washers | 2.00 | 5.5
| Modified Energy Factor (MEF) ft3/kWh/cycle | Integrated Water Factor (IWF) gal./ft3cycle
Effective January 1, 2018 | Effective January 1, 2018
Top-loading clothes washers | 1.35 | 8.8
Front-loading clothes washers | 2.00 | 4.1

### (q) Clothes Dryers.

(1) Energy Efficiency Standards for Vented Electric Clothes Dryers, Ventless Electric Clothes Dryers, and Vented Gas Clothes Dryers. The combined energy factor of vented electric clothes dryers that are consumer products, ventless electric clothes dryers that are consumer products, and vented gas clothes dryers that are consumer products, and that are manufactured on or after January 1, 2015 shall be not less than the applicable values shown in Table Q.

#### Table Q
Standards for Vented Electric Clothes Dryers, Ventless Electric Clothes Dryers, and
Vented Gas Clothes Dryers Manufactured On or After January 1, 2015

Appliance | Minimum Combined Energy Factor (lbs/kWh)
Vented | Ventless
Electric, standard clothes dryers | 3.73 | ---
Electric, compact, 120 volt clothes dryers | 3.61 | ---
Electric, compact, 240 volt clothes dryers | 3.27 | 2.55
Electric, combination washer-dryer | --- | 2.08
Gas clothes dryers | 3.30 | ---

### (r) Cooking Products and Food Service Equipment.

(1) Energy Design Standard for Gas Cooking Products.

(A) Gas Cooking Products Equipped with an Electrical Supply Cord. Gas cooking products that are consumer products and that are equipped with an electrical supply cord shall not be equipped with a constant burning pilot light.

(B) Gas Cooking Products Not Equipped with an Electrical Supply Cord. Gas cooking products that are consumer products manufactured on or after April 9, 2012, and that are not equipped with an electrical supply cord shall not be equipped with a constant burning pilot light.

(2) Microwave Ovens Manufactured On or After June 17, 2016.

Microwave-only ovens, countertop convection microwave ovens, built-in microwave ovens, and over-the-range convection microwave ovens manufactured on or after June 17, 2016 shall not exceed the average standby power rating (watts) shown in Table R-2..

#### Table R-2
Standards for Microwave Ovens Manufactured On or After June 17, 2016

Appliance | Maximum Standby Power (Watts)
Microwave-only oven | 1.0
Countertop convection microwave oven | 1.0
Built-in microwave oven | 2.2
Over‐the‐range convection microwave oven | 2.2

(3) Hot Food Holding Cabinets. See Section 1605.3(r) of this Article for energy ‘efficiency standards for commercial hot food holding cabinets.

(4) Other Cooking Products and Food Service Equipment. There is no energy efficiency standard or energy design standard for other cooking products or for food service equipment.

### (s) Electric Motors and Compressors.

(1) Standards for Electric Motors. The standards shown in Tables S-1, S-2, and S-3 of this Article apply only to electric motors, including partial electric motors that satisfy the following criteria:

(A) Are single-speed, induction motors;

(B) Are rated for continuous duty (MG 1) operation or for duty type S1 (IEC);

(C) Contain a squirrel-cage (MG 1) or cage (IEC) rotor;

(D) Operate on polyphase alternating current 60-hertz sinusoidal line power;

(E) Are rated 600 volts or less;

(F) Have a 2-, 4-, 6-, or 8-pole configuration,

(G) Are built in a three-digit or four-digit NEMA frame size (or IEC metric equivalent), including those designs between two consecutive NEMA frame sizes (or IEC metric equivalent), or an enclosed 56 NEMA frame size (or IEC metric equivalent),

(H) Produce at least one horsepower (0.746 kW) but not greater than 500 horsepower (373 kW), and

(I) Meet all of the performance requirements of one of the following motor types: A NEMA Design A, B, or C motor or an IEC Design N or H motor.

(2) NEMA Design A Motors, NEMA Design B Motors, and IEC Design N Motors. Starting on June 1, 2016, each NEMA Design A motor, NEMA Design B motor, and IEC Design N motor that is an electric motor meeting the criteria in section 1605.1(s)(1) of this Article and with a power rating from 1 horsepower through 500 horsepower, but excluding fire pump electric motors, manufactured (alone or as a component of another piece of equipment) shall have a nominal full-load efficiency of not less than the values shown in Table S-1:

#### Table S-1
Minimum Nominal Full-Load Efficiencies of NEMA Design A, NEMA Design B and
IEC Design N Motors (Excluding Fire Pump Electric Motors) at 60 Hz

Motor Horsepower/ Standard kilowatt equivalent | Nominal Full‐Load Efficiency(%)
2 pole | 4 pole | 6 pole | 8 pole
Enclosed | Open | Enclosed | Open | Enclosed | Open | Enclosed | Open
1/.75 | 77.0 | 77.0 | 85.5 | 85.5 | 82.5 | 82.5 | 75.5 | 75.5
1.5/1.1 | 84.0 | 84.0 | 86.5 | 86.5 | 87.5 | 86.5 | 78.5 | 77.0
2/1.5 | 85.5 | 85.5 | 86.5 | 86.5 | 88.5 | 87.5 | 84.0 | 86.5
3/2.2 | 86.5 | 85.5 | 89.5 | 89.5 | 89.5 | 88.5 | 85.5 | 87.5
5/3.7 | 88.5 | 86.5 | 89.5 | 89.5 | 89.5 | 89.5 | 86.5 | 88.5
7.5/5.5 | 89.5 | 88.5 | 91.7 | 91.0 | 91 | 90.2 | 86.5 | 89.5
10/7.5 | 90.2 | 89.5 | 91.7 | 91.7 | 91 | 91.7 | 89.5 | 90.2
15/11 | 91.0 | 90.2 | 92.4 | 93.0 | 91.7 | 91.7 | 89.5 | 90.2
20/15 | 91.0 | 91.0 | 93.0 | 93.0 | 91.7 | 92.4 | 90.2 | 91.0
25/18.5 | 91.7 | 91.7 | 93.6 | 93.6 | 93.0 | 93.0 | 90.2 | 91.0
30/22 | 91.7 | 91.7 | 93.6 | 94.1 | 93.0 | 93.6 | 91.7 | 91.7
40/30 | 92.4 | 92.4 | 94.1 | 94.1 | 94.1 | 94.1 | 91.7 | 91.7
50/37 | 93.0 | 93.0 | 94.5 | 94.5 | 94.1 | 94.1 | 92.4 | 92.4
60/45 | 93.6 | 93.6 | 95.0 | 95.0 | 94.5 | 94.5 | 92.4 | 93.0
75/55 | 93.6 | 93.6 | 95.4 | 95.0 | 94.5 | 94.5 | 93.6 | 94.1
100/75 | 94.1 | 93.6 | 95.4 | 95.4 | 95.0 | 95.0 | 93.6 | 94.1
125/90 | 95.0 | 94.1 | 95.4 | 95.4 | 95.0 | 95.0 | 94.1 | 94.1
150/110 | 95.0 | 94.1 | 95.8 | 95.8 | 95.8 | 95.4 | 94.1 | 94.1
200/150 | 95.4 | 95.0 | 96.2 | 95.8 | 95.8 | 95.4 | 94.5 | 94.1
250/186 | 95.8 | 95.0 | 96.2 | 95.8 | 95.8 | 95.8 | 95.0 | 95.0
300/224 | 95.8 | 95.4 | 96.2 | 95.8 | 95.8 | 95.8 |  |
350/261 | 95.8 | 95.4 | 96.2 | 95.8 | 95.8 | 95.8 |  |
400/298 | 95.8 | 95.8 | 96.2 | 95.8 |  |  |  |
450/336 | 95.8 | 96.2 | 96.2 | 96.2 |  |  |  |
500/373 | 95.8 | 96.2 | 96.2 | 96.2 |  |  |  |

(3) NEMA Design C motors and IEC Design H motors. Starting on June 1, 2016, each NEMA Design C motor and IEC Design H motor that is an electric motor meeting the criteria in section 1605.1(s)(1) of this Article and with a power rating from 1 horsepower through 200 horsepower manufactured (alone or as a component of another piece of equipment) shall have a nominal full-load efficiency that is not less than the values shown in Table S-2:

#### Table S-2
Minimum Nominal Full-Load Efficiencies of NEMA Design C and IEC Design H Motors at 60 Hz

Motor Horsepower/ Standard Kilowatt Equivalent | Nominal Full‐Load Efficiency(%)
4 pole | 6 pole | 8 pole
Enclosed | Open | Enclosed | Open | Enclosed | Open
1/.75 | 85.5 | 85.5 | 82.5 | 82.5 | 75.5 | 75.5
1.5/1.1 | 86.5 | 86.5 | 87.5 | 86.5 | 78.5 | 77.0
2/1.5 | 86.5 | 86.5 | 88.5 | 87.5 | 84.0 | 86.5
3/2.2 | 89.5 | 89.5 | 89.5 | 88.5 | 85.5 | 87.5
5/3.7 | 89.5 | 89.5 | 89.5 | 89.5 | 86.5 | 88.5
7.5/5.5 | 91.7 | 91.0 | 91 | 90.2 | 86.5 | 89.5
10/7.5 | 91.7 | 91.7 | 91 | 91.7 | 89.5 | 90.2
15/11 | 92.4 | 93.0 | 91.7 | 91.7 | 89.5 | 90.2
20/15 | 93.0 | 93.0 | 91.7 | 92.4 | 90.2 | 91.0
25/18.5 | 93.6 | 93.6 | 93.0 | 93.0 | 90.2 | 91.0
30/22 | 93.6 | 94.1 | 93.0 | 93.6 | 91.7 | 91.7
40/30 | 94.1 | 94.1 | 94.1 | 94.1 | 91.7 | 91.7
50/37 | 94.5 | 94.5 | 94.1 | 94.1 | 92.4 | 92.4
60/45 | 95.0 | 95.0 | 94.5 | 94.5 | 92.4 | 93.0
75/55 | 95.4 | 95.0 | 94.5 | 94.5 | 93.6 | 94.1
100/75 | 95.4 | 95.4 | 95.0 | 95.0 | 93.6 | 94.1
125/90 | 95.4 | 95.4 | 95.0 | 95.0 | 94.1 | 94.1
150/110 | 95.8 | 95.8 | 95.8 | 95.4 | 94.1 | 94.1
200/150 | 96.2 | 95.8 | 95.8 | 95.4 | 94.5 | 94.1

(4) Fire Pump Electric Motors. Starting on June 1, 2016, each fire pump electric motor meeting the criteria in section 1605.1(s)(1) of this Article and with a power rating of 1 horsepower through 500 horsepower, manufactured (alone or as a component of another piece of equipment) shall have a nominal full-load efficiency that is not less than the values shown in Table S-3

#### Table S-3
Minimum Nominal Full-Load Efficiencies of Fire Pump Electric Motors at 60 Hz

Motor Horsepower/ Standard Kilowatt Equivalent | Nominal Full‐Load Efficiency(%)
2 pole | 4 pole | 6 pole | 8 pole
Enclosed | Open | Enclosed | Open | Enclosed | Open | Enclosed | Open
1/.75 | 75.5 |  | 82.5 | 82.5 | 80.0 | 80.0 | 74.0 | 74.0
1.5/1.1 | 82.5 | 82.5 | 84.0 | 84.0 | 85.5 | 84.0 | 77.0 | 75.5
2/1.5 | 84.0 | 84.0 | 84.0 | 84.0 | 86.5 | 85.5 | 82.5 | 85.5
3/2.2 | 85.5 | 84.0 | 87.5 | 86.5 | 87.5 | 86.5 | 84.0 | 86.5
5/3.7 | 87.5 | 85.5 | 87.5 | 87.5 | 87.5 | 87.5 | 85.5 | 87.5
7.5/5.5 | 88.5 | 87.5 | 89.5 | 88.5 | 89.5 | 88.5 | 85.5 | 88.5
10/7.5 | 89.5 | 88.5 | 89.5 | 89.5 | 89.5 | 90.2 | 88.5 | 89.5
15/11 | 90.2 | 89.5 | 91.0 | 91.0 | 90.2 | 90.2 | 88.8 | 89.5
20/15 | 90.2 | 90.2 | 91.0 | 91.0 | 90.2 | 91.0 | 89.5 | 90.2
25/18.5 | 91.0 | 91.0 | 92.4 | 91.7 | 91.7 | 91.7 | 89.5 | 90.2
30/22 | 91.0 | 91.0 | 92.4 | 92.4 | 91.7 | 92.4 | 91.0 | 91.0
40/30 | 91.7 | 91.7 | 93.0 | 93.0 | 93.0 | 93.0 | 91.0 | 91.0
50/37 | 92.4 | 92.4 | 93.0 | 93.0 | 93.0 | 93.0 | 91.7 | 91.7
60/45 | 93.0 | 93.0 | 93.6 | 93.6 | 93.6 | 93.6 | 91.7 | 92.4
75/55 | 93.0 | 93.0 | 94.1 | 94.1 | 93.6 | 93.6 | 93.0 | 93.6
100/75 | 93.6 | 93.0 | 94.5 | 94.1 | 94.1 | 94.1 | 93.0 | 93.6
125/90 | 94.5 | 93.6 | 94.5 | 94.5 | 94.1 | 94.1 | 93.6 | 93.6
150/110 | 94.5 | 93.6 | 95.0 | 95.0 | 95.0 | 94.5 | 93.6 | 93.6
200/150 | 95.0 | 94.5 | 95.0 | 95.0 | 95.0 | 94.5 | 94.1 | 93.6
250/186 | 95.4 | 94.5 | 95.0 | 95.4 | 95.0 | 95.4 | 94.5 | 94.5
300/224 | 95.4 | 95.0 | 95.4 | 95.4 | 95.0 | 95.4 |  |
350/261 | 95.4 | 95.0 | 95.4 | 95.4 | 95.0 | 95.4 |  |
400/298 | 95.4 | 95.4 | 95.4 | 95.4 |  |  |  |
450/336 | 95.4 | 95.8 | 95.4 | 95.8 |  |  |  |
500/373 | 95.4 | 95.8 | 95.8 | 95.8 |  |  |  |

EXCEPTION to Sections 1605.1(s)(2), 1605.1(s)(3), and 1605.1(s)(4) of this Article. The standards in Tables S-1, S-2 or S-3 of this Article do not apply to the following electric motors exempted by the Secretary, or any additional electric motors that the Secretary may exempt:

(A) Air-over electric motors;

(B) Component sets of an electric motor;

(C) Liquid-cooled electric motors;

(D) Submersible electric motors; and

(E) Inverter-only electric motors.

(5) Small Electric Motors. The average full load efficiency of each small open electric motor manufactured (alone or as a component of another piece of non‐covered equipment) after March 9, 2015, or in the case of a ‘small electric motor which requires listing or certification by a nationally recognized safety testing laboratory, after March 9, 2017, shall be not less than the values shown in Table S‐4:

#### Table S-4
Standards for Small Electric Motors

Motor Horsepower/ Standard Kilowatt Equivalent | Minimum Average Full‐Load Efficiency
Polyphase | Capacitor‐start capacitor‐run and capacitor‐start induction run Motors
6 poles | 4 poles | 2 poles | 6 poles | 4 poles | 2 poles
0.25/0.18 | 67.5 | 69.5 | 65.6 | 62.2 | 68.5 | 66.6
0.33/0.25 | 71.4 | 73.4 | 69.5 | 66.6 | 72.4 | 70.5
0.5/0.37 | 75.3 | 78.2 | 73.4 | 76.2 | 76.2 | 72.4
0.75/0.55 | 81.7 | 81.1 | 76.8 | 80.2 | 81.8 | 76.2
1.0/0.75 | 82.5 | 83.5 | 77.0 | 81.1 | 82.6 | 80.4
1.5/1.1 | 83.8 | 86.5 | 84.0 |  | 83.8 | 81.5
2.0/1.5 |  | 86.5 | 85.5 |  | 84.5 | 82.9
3.0/2.2 |  | 86.9 | 85.5 |  |  | 84.1

6) Determinations of Efficiency. For purposes of determining the required minimum nominal full load efficiency of an electric motor that has a horsepower or kilowatt rating between two horsepower or two kilowatt ratings shown in Tables S-1, S-2, or S-3, or of determining the required minimum average full load efficiency of a small electric motor that has a horsepower or kilowatt rating between two horsepower or kilowatt ratings shown in Table S-4, each such motor shall be deemed to have a listed horsepower or kilowatt rating determined as follows:

(A) A horsepower at or above the midpoint between the two consecutive horsepower ratings shall be rounded up to the higher of the two horsepower ratings;

(B) A horsepower below the midpoint between the two consecutive horsepower ratings shall be rounded down to the lower of the two horsepower ratings; or

(C) A kilowatt rating shall be directly converted from kilowatts to horsepower using the formula, 1 kilowatt = (1/0.746) horsepower, without calculating beyond three significant decimal places, and the resulting horsepower shall be rounded in accordance with sections 1605.1(s)(6)(A) or 1605.1(s)(6)(B) of this Article, whichever applies.

(7) Compressors.

(A) Federally Regulated Compressors. Federally regulated compressors manufactured on

or after January 10, 2025, shall meet the applicable energy efficiency standards in Table

S-5.

#### Table S-5
Standards for Federally Regulated Compressors Manufactured on or After January 10, 2025

Equipment Class | Minimum Package Isentropic Efficiency† | ηRegr (package isentropic efficiency reference curve) | d (Percentage Loss Reduction
Rotary, lubricated, air-cooled, fixed-speed compressor | ????egr + (1 − ????egr ) * (d/100) | −0.00928 ∗ ln2(. 4719 ∗ ??1) + 0.13911 ∗ ln(. 4719 ∗ ??1) + 0.27110 | -15
Rotary, lubricated, air-cooled, variable-speed compressor | ????egr + (1 − ????egr ) * (d/100) | −0.01549 ∗ ln2(. 4719 ∗ ??1) + 0.21573 ∗ ln(. 4719 ∗ ??1) + 0.00905 | -10
Rotary, lubricated, liquid-cooled, fixed-speed compressor | .02349 + ????egr + (1 − ??��egr ) * d/100) | −0.00928 ∗ ln2(. 4719 ∗ ??1) + 0.13911 ∗ ln(. 4719 ∗ ??1) + 0.27110 | -15
Rotary, lubricated, liquid-cooled, variable-speed compressor | .02349 + ????egr + (1 − ????egr ) * (d/100) | −0.01549 ∗ ln2(. 4719 ∗ ??1) + 0.21573 ∗ ln(. 4719 ∗ ??1) + 0.00905 | -15
Where V1 is the full-load actual volume flow rate of the compressor, in cubic feet per minute, as determined in accordance with the test procedure in section 1604(s) of this Article. † For “fixed-speed compressor” equipment classes, the relevant Package Isentropic Efficiency is Full-load Package Isentropic Efficiency. For “Variable-speed compressor” equipment classes, the relevant Package Isentropic Efficiency is Part-load Package Isentropic Efficiency. Both Full- and Part-Load Package Isentropic Efficiency are determined in accordance with the test procedure in section 1604(s) of this Article.

(B) State-Regulated Compressors. See section 1605.3(s) of this Article for energy efficiency

standards for state-regulated compressors manufactured on or after January 1, 2022,

but prior to January 10, 2025.

### (t) Distribution Transformers.

(1) Low‐Voltage Dry‐Type Distribution Transformers. The ‘efficiency of a low‐voltage dry‐ type distribution ‘transformer manufactured on or after January 1, 2016 shall be not less than that required for their kVA rating as shown in Table T‐3. Low‐voltage dry‐type distribution transformers with kVA ratings not appearing in Table T‐3 shall have their minimum efficiency determined by linear interpolation of the kVA and efficiency values immediately above and below that kVA rating.

#### Table T-3
Standards for Low-Voltage Dry-Type Distribution Transformers

Single phase | Three phase
kVa | ‘Efficiency (%)¹ | kVa | ‘Efficiency (%)¹
15 | 97.7 | 15 | 97.89
25 | 98.0 | 30 | 98.23
37.5 | 98.2 | 45 | 98.40
50 | 98.3 | 75 | 98.60
75 | 98.5 | 112.5 | 98.74
100 | 98.6 | 150 | 98.83
167 | 98.7 | 225 | 98.94
250 | 98.8 | 300 | 99.02
333 | 98.9 | 500 | 99.14
|  | 750 | 99.23
|  | 1000 | 99.28
¹ All efficiency values are at 35 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under Appendix A to subpart K of 10 C.F.R. part 431.
|  |  |  |  |

(2) Liquid‐Immersed Distribution Transformers. The efficiency of a liquid‐ immersed distribution ‘transformer manufactured on or after January 1, 2016 shall be no less than that required for their kVA rating as shown in Table T‐4. Liquid‐immersed distribution transformers with kVA ratings not appearing in Table T‐4 shall have their minimum efficiency level determined by linear interpolation of the kVA and efficiency values immediately above and below that kVA rating.

#### Table T-4
Standards for Liquid-Immersed Distribution Transformers

Single phase | Three phase
kVA | ‘Efficiency (%)¹ | kVA | ‘Efficiency (%)¹
10 | 98.70 | 15 | 98.65
15 | 98.82 | 30 | 98.83
25 | 98.95 | 45 | 98.92
37.5 | 99.05 | 75 | 99.03
50 | 99.11 | 112.5 | 99.11
75 | 99.19 | 150 | 99.16
100 | 99.25 | 225 | 99.23
167 | 99.33 | 300 | 99.27
250 | 99.39 | 500 | 99.35
333 | 99.43 | 750 | 99.40
500 | 99.49 | 1000 | 99.43
667 | 99.52 | 1500 | 99.48
833 | 99.55 | 2000 | 99.51
|  | 2500 | 99.53
¹ All efficiency values are at 50 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under Appendix A to subpart K of 10 C.F.R. part 431.

(3) Medium‐Voltage Dry‐Type Distribution Transformers. The efficiency of a medium‐ voltage dry‐type distribution ‘transformer manufactured on or after January 1, 2016, shall be no less than that required for their kVA and BIL rating in Table T‐5. Medium‐ voltage dry‐type distribution ‘transformers with kVA ratings not appearing in Table T‐5 shall have their minimum efficiency level determined by linear interpolation of the kVA and efficiency values immediately above and below that kVA rating.

#### Table T-5
Standards for Medium-Voltage Dry-Type Distribution Transformers
Manufactured On or After January 1, 2016

Single phase | Three phase
BIL | BIL
kVA | 20‐45 kV efficiency¹ (%) | 46‐95 kV efficiency¹ (%) | ≥ 96 kV efficiency¹ (%) | BIL kVA | 20‐45 kV efficiency¹ (%) | 46‐95 kV efficiency¹ (%) | ≥ 96 kV efficiency¹ (%)
15 | 98.10 | 97.86 |  | 15 | 97.50 | 97.18 |
25 | 98.33 | 98.12 |  | 30 | 97.90 | 97.63 |
37.5 | 98.49 | 98.30 |  | 45 | 98.10 | 97.86 |
50 | 98.60 | 98.42 |  | 75 | 98.33 | 98.13 |
75 | 98.73 | 98.57 | 98.53 | 112.5 | 98.52 | 98.36 |
100 | 98.82 | 98.67 | 98.63 | 150 | 98.65 | 98.51 |
167 | 98.96 | 98.83 | 98.80 | 225 | 98.82 | 98.69 | 98.57
250 | 99.07 | 98.95 | 98.91 | 300 | 98.93 | 98.81 | 98.69
333 | 99.14 | 99.03 | 98.99 | 500 | 99.09 | 98.99 | 98.89
500 | 99.22 | 99.12 | 99.09 | 750 | 99.21 | 99.12 | 99.02
667 | 99.27 | 99.18 | 99.15 | 1000 | 99.28 | 99.20 | 99.11
833 | 99.31 | 99.23 | 99.20 | 1500 | 99.37 | 99.30 | 99.21
|  |  |  | 2000 | 99.43 | 99.36 | 99.28
|  |  |  | 2500 | 99.47 | 99.41 | 99.33
¹ All efficiency values are at 50 percent of nameplate-rated load, determined according to the DOE Test Method for Measuring the Energy Consumption of distribution Transformers under Appendix A to subpart K of 10 C.F.R. part 431

### (u) External Power Supplies.

(1) Class A External Power Supplies. Except as provided in subsections 1605.1(u)(4) and 1605.1(u)(7) of this Article, all Class A external power supplies manufactured on or after July 1, 2008 shall meet the standards shown in Table U-1:

#### Table U-1
Standards for Class A External Power Supplies

Active Mode
Nameplate ‘Output | Required efficiency (decimal equivalent of a percentage)
Less than 1 watt | 0.5 times theNameplate Output
From 1 watt to not more than 51 watts | The sum of 0.09 times the Natural Logarithm of the Nameplate Output and 0.5
Greater than 51 watts | 0.85
Not more than 250 watts | No-Load Mode
Maximum Consumption
0.5 Watts

(2) Direct Operation External Power Supplies. Except as provided in subsections 1605.1(u)(7) and 1605.1(u)(8) of this Article, all direct operation external power supplies manufactured on or after February 10, 2016, shall meet the standards shown in Table U-2:

#### Table U-2
Standards for Direct Operation External Power Supplies

Power Supply Type | Nameplate ‘Output Power (Pout) | Minimum Average ‘Efficiency in Active Mode* | Maximum Power in No-Load Mode [W]
Single-Voltage External AC-DC Power Supply, Basic Voltage | Pout ≤ 1 W | ≥ 0.5 x Pout + 0.16 | ≤ 0.100
1 W ≤ Pout ≤ 49 W | ≥ 0.071 x In(Pout) - 0.0014 x Pout +0.67 | ≤ 0.100
49 W ≤ Pout ≤ 250 W | ≥ 0.880 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-DC Power Supply, Low-Voltage | Pout ≤ 1 W | ≥ 0.517 x Pout + 0.087 | ≤ 0.100
1 W ≤ Pout ≤ 49 W | ≥ 0.0834 x In(Pout) - 0.0014 x Pout +0.609 | ≤ 0.100
49 W ≤ Pout ≤ 250 W | ≥ 0.870 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-AC Power Supply, Basic Voltage | Pout ≤ 1 W | ≥ 0.5 x Pout + 0.16 | ≤ 0.210
1 W ≤ Pout ≤ 49 W | ≥ 0.071 x In(Pout) - 0.0014 x Pout +0.67 | ≤ 0.210
49 W < Pout ≤ 250 W | ≥ 0.880 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Single-Voltage External AC-AC Power Supply, Low-Voltage | Pout ≤ 1 W | ≥ 0.517 x Pout + 0.087 | ≤ 0.210
1 W ≤ Pout ≤ 49 W | ≥ 0.0834 x In(Pout) - 0.0014 x Pout +0.609 | ≤ 0.210
49 W ≤ Pout ≤ 250 W | ≥ 0.870 | ≤ 0.210
Pout >250 W | ≥ 0.875 | ≤ 0.500
Multiple-Voltage External Power Supply | Pout ≤ 1 W | ≥ 0.497 x Pout + 0.067 | ≤ 0.300
1 W < Pout ≤ 49 W | ≥ 0.075 x In(Pout) +0.561 | ≤ 0.300
Pout > 49W | ≥ 0.860 | ≤ 0.300
*Expressed as a decimal

(3) All External Power Supplies Manufactured On or After February 10, 2016. Except as provided in subsections 1605.1(u)(7) and 1605.1(u)(8) of this Article, all direct operation external power supplies manufactured on or after February 10, 2016, shall meet the standards shown in Table U-3:

#### Table U-3
Standards for All External Power Supplies Manufactured On or After February 10, 2016

Operation EPS Type | Class A EPS | Non-Class A EPS
Direct Operation EPS | Level VI: 10 C.F.R. 430.32 (w)(1)(ii) | Level VI: 10 C.F.R. 430.32 (w)(1)(ii)
Indirect Operation EPS | Level VI: 10 C.F.R. 430.32 (w)(1)(i) | No standards

(4) Exclusions. A basic model of external power supply is not subject to the energy conservation standards of section 1605.1(u)(2) of this Article if the external power supply:

(A) Is manufactured during the period beginning on February 10, 2016, and ending on February 10, 2020;

(B) Is marked in accordance with the External Power Supply International Efficiency Marking Protocol, as in effect on February 10, 2016;

(C) Meets, where applicable, the standards under section 1605.1(u)(1) of this Article, and has been certified to the Secretary as meeting those standards; and

(D) Is made available by the manufacturer only as a service part or a spare part for an end-use product that:

1. constitutes the primary load; and

2. was manufactured before February 10, 2016.

(5) End Use Product Exclusion. The standards described in sections 1605.1(u)(1), 1605.1(u)(2), and 1605.1(u)(3) of this Article shall not constitute an energy conservation standard for the separate end-use product to which the external power supply is connected.

(6) Non-application of no-load mode requirements. The no-load mode energy efficiency standards established in sections 1605.1(u)(1), 1605.1(u)(2), and 1605.1(u)(3) of this Article shall not apply to an external power supply manufactured before July 1, 2017, that:

(A) Is an AC-to-AC external power supply;

(B) Has a nameplate output of 20 watts or more;

(C) Is certified to the Secretary as being designed to be connected to a security or life safety alarm or surveillance system component; and

(D) On establishment within the External Power Supply International Efficiency Marking Protocol, as referenced in the “Energy Star Program Requirements for Single Voltage External Ac-Dc and Ac-Ac Power Supplies” (incorporated by reference in 10 C.F.R. section 430.3), published by the Environmental Protection Agency, of a distinguishing mark for products described in this clause, is permanently marked with the distinguishing mark.

(7) FDA Listing. An external power supply shall not be subject to the standards in sections 1605.1(u)(1), 1605.1(u)(2), and 1605.1(u)(3) of this Article if it is a device that requires Federal Food and Drug Administration (FDA) listing and approval as a medical device in accordance with section 513 of the Federal Food, Drug, and Cosmetic Act (21 U.S.C. 360(c)).

8) Exclusion of Battery Chargers Used in a Product that is Fully or Primarily Motor Operated. A direct operation, AC-DC external power supply with nameplate output voltage less than 3 volts and nameplate output current greater than or equal to 1,000 milliamps that charges the battery of a product that is fully or primarily motor operated shall not be subject to the standards in section 1605.1(u)(2) of this Article.

### (v) Computers, Computer Monitors, Televisions, Signage Displays, and Consumer Audio and Video Equipment.

See Section 1605.3(v) of this Article for energy ‘efficiency standards for computers, computer monitors, televisions, signage displays, and consumer audio and video equipment.

### (w) Battery Chargers and Battery Charger Systems.

(1) Federally Regulated Battery Chargers Manufactured on or after June 13, 2018. Federally regulated battery chargers manufactured on or after June 13, 2018 must have a unit energy consumption (UEC) less than or equal to the prescribed “Maximum UEC” standard when using the equations for the appropriate product class and corresponding rated battery energy as shown in Table W-1:

#### Table W-1
Standards for Federally Regulated Battery Chargers
Manufactured on or after June 13, 2018

Product Class | Product Class Description | Rated Battery Energy (Ebatt**) | Special Characteristic or battery voltage | Maximum UEC (kWh/yr) (as a function of Ebatt**)
1 | Low-Energy | ≤ 5 Wh | Inductive Connection* | 3.04
2 | Low-Energy Low-Voltage | < 100 Wh | < 4 V | 0.1440 * Ebatt + 2.95
3 | Low-Energy Medium-Voltage | < 100 Wh | ≥ 4 V and ≤ 10V | For Ebatt <10 Wh, 1.42 kWh/yr. For Ebatt ≥10 Wh, 0.0255 * Ebatt + 1.16
4 | Low-Energy High-Voltage | < 100 Wh | > 10 V | 0.11 * Ebatt + 3.18
5 | Medium-Energy Low-Voltage | ≥ 100 Wh and ≤ 3,000 Wh | < 20 V | 0.0257 * Ebatt + 0.815
6 | Medium-Energy High-Voltage | ≥ 100 Wh and ≤ 3,000 Wh | ≥ 20 V | 0.0778 * Ebatt + 2.4
7 | High-Energy | >3,000 Wh |  | 0.0502 * Ebatt + 4.53
*Inductive connection and designed for use in a wet environment (e.g. electric toothbrushes). **Ebatt = Rated battery energy as determined in 10 C.F.R.part 429.39(a).

Exception: to Battery Charger Standards in section 1605.1(w)(1) of this Article. A battery charger shall not be subject to the standards in section 1605.1(w)(1) of this Article if it is a device that requires Federal Food and Drug Administration (FDA) listing and approval as a life-sustaining or life-supporting device in accordance with section 513 of the Federal Food, Drug, and Cosmetic Act (21 U.S.C. 360(c)).

(2) Federally Regulated Uninterruptible Power Supplies (UPSs) Manufactured on and after

January 10, 2022. Federally regulated uninterruptible power supplies manufactured on or

after January 10, 2022, that utilize a NEMA 1-15P or 5-15P input plug and have an AC

output shall have an average load adjusted efficiency that meets or exceeds the values

shown in Table W-2 based on the rated output power (Prated) of the UPS.

#### Table W-2
Standards for Federally Regulated Uninterruptible Power Supplies (UPS)

#### Manufactured on or after January 10, 2022

Battery charger product class | Rated output power | Minimum efficiency
10a (VFD UPSs) | 0 W < Prated ≤ 300 W | −1.20E-06 * P2rated + 7.17E-04 * Prated + 0.862
300 W < Prated ≤ 700 W | −7.85E-08 * P2rated + 1.01E-04 * Prated + 0.946
Prated > 700 W | −7.23E-09 * P2rated + 7.52E-06 * Prated + 0.977
10b (VI UPSs) | 0 W < Prated ≤ 300 W | −1.20E-06 * P2rated + 7.19E-04 * Prated + 0.863
300 W < Prated ≤ 700 W | −7.67E-08 * P2rated + 1.05E-04 * Prated + 0.947
Prated > 700 W | −4.62E-09 * P2rated + 8.54E-06 * Prated + 0.979
10c (VFI UPSs) | 0 W < Prated ≤ 300 W | −3.13E-06 * P2rated + 1.96E-03 * Prated + 0.543
| 300 W < Prated ≤ 700 W | −2.60E-07 * P2rated + 3.65E-04 * Prated + 0.764
| Prated > 700 W | −1.70E-08 * P2rated + 3.85E-05 * Prated + 0.876

(3) See section 1605.3(w) of this Article for energy efficiency standards for battery charger

systems.

### (x) Landscape irrigation equipment.

See section 1605.3(x) of this Article for water efficiency standards for landscape irrigation equipment.

The following documents are incorporated by reference in section 1605.1.

FEDERAL STATUTES AND REGULATIONS

C.F.R., Title 10, section 429.39(a)

C.F.R., Title 10, section 429.44

C.F.R., Title 10, section 429.59

C.F.R., Title 10, part 430, subpart B, appendix AA

C.F.R., Title 10, part 430.2

C.F.R., Title 10, part 430.3

C.F.R., Title 10, sections 430.23(a) (Appendix A to subpart B of part 430)

C.F.R., Title 10, sections 430.23(b) (Appendix B to subpart B of part 430)

C.F.R., Title 10, section 430.32(c)

C.F.R., Title 10, section 430.32(d)

C.F.R., Title 10, section 430.32(w)(1)

C.F.R., Title 10, sections 431.63

C.F.R., Title 10, sections 431.66(d)(2)(i) through (iii)

C.F.R., Title 10, section 431.110

C.F.R., Title 10, section 431.324

C.F.R., Title 10, section 431.326(b)(3)

C.F.R., Title 10, section 431.462

C.F.R., Title 10, part 431, subpart K, Appendix A

C.F.R., Title 10, section 431.465(c)(6)

C.F.R., Title 10, part 431, subpart Y, Appendix A, Section II.B

C.F.R., Title 10, part 50, “Domestic Licensing of Production and Utilization Facilities”

Copies available from: | Superintendent of Documents |
| U.S. Government Printing Office |
| Washington, DC 20402 |
| http://www.ecfr.gov |
UNITED STATES ENVIRONMENTAL PROTECTION AGENCY (EPA) |
| EPA “External ‘Power Supply International Efficiency Marking Protocol” |
Copies available from: | US EPA |
| Climate Protection Partnership |
| ENERGY STAR Programs Hotline & |
| Distribution |
| (MS- 6202 J) |
| 1200 Pennsylvania Ave NW |
| Washington, ‘DC 20460 |
| www.energystar.gov |
AIR-CONDITIONING, HEATING, AND REFRIGERATION INSTITUTE (AHRI) |
AHRI 1200-2006 | Performance Rating of Commercial Refrigerated Display Merchandisers and Storage Cabinets |
Copies available from: | Air-Conditioning, Heating and |
| Refrigeration Institute (AHRI) |
| 2111 Wilson Blvd, Suite 500 |
| Arlington, VA 22201 |
| Phone: (703) 524-8800 |
| FAX: (703) 562-1942 |
| http://www.ahrinet.org |
AMERICAN NATIONAL STANDARDS INSTITUTE (ANSI) |
ANSI C78.5 | Standard for Electric Lamps - Specifications for Performance of Self-Ballasted Compact Fluorescent Lamps |
Copies available from: | American National Standards Institute |
| 1819 L Street, NW, 6th Floor |
| Washington, DC 2003 6 |
| www.ansi.org |
| Phone: (202) 293-8020 |
| FAX: (202) 293-9287 |
ILLUMINATING ENGINGEERING SOCIETY (IES) |
IES LM-65 | Life Testing of Compact Fluorescent Lamps |
Copies available from: | Illuminating Engineering Society |
| 120 Wall Street, 17th Floor |
| New York, NY 10005-4001 |
| www.ies.org |
| Phone: (212) 248-5000 |
| FAX: (212) 248-5017/18 |
NATIONAL ELECTRIC CODE (NEC) |
NFPA 70 (2002) | National Electrical Code section 410.4(A) |
Copies available from: | National Fire Protection Association |
| 1 Batterymarch Park |
| Quincy, MA 02169-7471 |
| www.nfpa.org |
| Phone: (617) 770-3000 |
| FAX: (617) 770-0700 |
NATIONAL ELECTRIC ‘MANUFACTURERS ASSOCIATION (NEMA) |
NEMA Standard TP-1-2002, Table 4-2 | Guide for Determining Energy Efficiency of Distribution ‘Transformers |
Copies available from: | National Electric Manufacturers Association |
| 1300 N. 17th Street, Suite 1847 |
| Rosslyn, VA 22209 |
| www.nema.org |
| Phone: (703) 841-3200 |
| FAX: (703) 81-3300 |
UNDERWRITERS LABS (UL) |
UL 1029-2001 | Standard for High-Intensity-Discharge Lamp Ballasts |
Copies available from: | Underwriters Laboratories, Inc. |
| 333 Pfingsten Road |
| Northbrook, IL 60062-2096 |
| www.ul.com |
| Phone: (847) 272-8800 |
| FAX: (847) 272-8129 |
|  |  |  |

Note: Authority cited: Sections 25213, 25218(e), 25401.9, 25402(a)-25402(c), and 25960, Public Resources Code; and sections 16, 26, and 30, Governor's Exec. Order No. B-29-15 (April 1, 2015). Reference: Sections 25216.5(d), 25401.9, 25402(a)-25402(c), and 25960, Public Resources Code; and Section 16, Governor's Exec. Order No. B-29-15 (April 1, 2015).

HISTORY

1. New section filed 10-28-2002; operative 11-27-2002 (Register 2002, No. 44).

2. Amendment of subsection (c)(1) Table C-2 filed 4-1-2003 as an emergency; operative 4-1-2003 (Register 2003, No. 14). A Certificate of Compliance must be transmitted to OAL by 7-30-2003 or emergency language will be repealed by operation of law on the following day.

3. Certificate of Compliance as to 4-1-2003 order transmitted to OAL 7-8-2003 and filed 8-19-2003 (Register 2003, No. 34).

4. Amendment of subsection (p)(1), new subsection (p)(4) and subsection renumbering filed 7-29-2004; operative 8-28-2004 (Register 2004, No. 31).

5. Amendment filed 3-16-2005; operative 4-15-2005 (Register 2005, No. 11).

6. Repealer of subsection (c)(2), subsection renumbering, amendment of subsection (f)(1), repealer of Table F-2, renumbering of tables, including amendment of newly designated Table F-2 and F-3 headings, and amendment of subsections (f)(2), (k)-(k)(3) and (u) and list of incorporated documents filed 12-30-2005; operative 1-1-2006 pursuant to Government Code section 11343.4 (Register 2005, No. 52).

7. Amendment of Note filed 12-14-2006; operative 12-14-2006 pursuant to Government Code section 11343.4 (Register 2006, No. 50).

8. Amendment filed 7-10-2009; operative 8-9-2009 (Register 2009, No. 28).

9. Amendment of subsection (l) and new subsections (l)(1)-(2) filed 10-26-2012; operative 1-1-2013 (Register 2012, No. 43).

10. Amendment filed 4-22-2014; operative 7-1-2014 (Register 2014, No. 17).

11. Amendment of subsection (h)(1) (including amendment of Table H-1), new subsection (h)(5), amendment of subsection (i) (including repealer of Table I) and amendment of Note filed with the Secretary of State by the Office of Administrative Law on 5-15-2015. Submitted to OAL for printing only pursuant to Governor's Executive Order No. B-29-15 (4-1-2015); operative 5-15-2015 (Register 2015, No. 20).

12. Amendment of subsections (h)(1) and (h)(5) and list of incorporated documents filed 8-20-2015; operative 8-20-2015 pursuant to Governor's Executive Order No. B-29-15, directive 30 (4-1-2015) (Register 2015, No. 34).

13. Amendment of subsections (a)(1), (a)(2)(A) and (a)(3), new subsections (a)(3)(A)-(C), amendment of subsection (a)(4)(C), new subsections (a)(4)(C)(i)-(ii), amendment of subsection (a)(6), repealer of subsection (b)(2)(A), subsection relettering, amendment of newly designated subsection (b)(2)(A) and subsections (c)(1)-(c)(1)(A), new subsection (c)(4), amendment of subsections (e)(1), (f)(2), (j) and (k)(2)(A)2.b.-c., new subsection (k)(2)(A)2.d., repealer and new subsections (n)(2)-(n)(3), amendment of subsections (p)(3) and (r)(2), new subsections (u)(1)(D)-(u)(1)(D)2. and amendment of subsection (w) filed 6-30-2016; operative 7-1-2016 pursuant to Government Code section 11343.4(b)(3) (Register 2016, No. 27).

14. Amendment of subsections within subsection (k), including renumbering of tables K-1 through K-8 to K-2 through K-9, filed 11-1-2016; operative 1-1-2017 (Register 2016, No. 45).

15. Amendment of subsection (v) filed 8-22-2017; operative 10-1-2017 (Register 2017, No. 34).

16. Amendment filed 9-26-2018; operative 10-1-2018 pursuant to Government Code section 11343.4(b)(3) (Register 2018, No. 39).

17. Editorial correction of subsections (a)(2)(C)2. and (c)(1)(A), Table O and subsection (w)(1) (Register 2018, No. 45).

18. Editorial correction of Table E-3 (Register 2018, No. 48).

19. Change without regulatory effect amending subsections (d)(4)-(d)(4)(A), Table F-4, subsections (g)(6)(C) and (j)(2)(D)2. and heading for Table K-3 filed 3-18-2019 pursuant to section 100, title 1, California Code of Regulations (Register 2019, No. 12).

20. New subsection (d)(5), subsection renumbering and amendment of newly designated subsection (d)(6) filed 3-18-2019; operative 3-18-2019 pursuant to Government Code section 11343.4(b)(3) (Register 2019, No. 12).

21. Amendment of subsection (s)(7) filed 6-10-2019; operative 6-10-2019 pursuant to Government Code section 11343.4(b)(3) (Register 2019, No. 24).

22. Change without regulatory effect amending Table C-3 filed 7-24-2019 pursuant to section 100, title 1, California Code of Regulations (Register 2019, No. 30).

23. New subsection (x) and amendment of Note filed 10-7-2019; operative 10-1-2020 pursuant to Government Code section 11343.4(b)(2) and Public Resources Code section 25402(c)(1) (Register 2019, No. 41).

24. Change without regulatory effect amending subsection (g)(6)(B)2. filed 12-12-2019 pursuant to section 100, title 1, California Code of Regulations (Register 2019, No. 50).

25. Amendment of subsections and tables within subsection (k) filed 12-24-2019; operative 1-1-2020 pursuant to Government Code section 11343.4(b)(3) (Register 2019, No. 52).

26. Amendment of subsections (g) and (g)(6)(A), new subsections (g)(7)-(g)(7)(E), subsection renumbering and amendment of newly designated subsection (g)(8) filed 9-21-2020; operative 1-1-2021 (Register 2020, No. 39). Filing deadline specified in Government Code section 11349.3(a) extended 60 calendar days pursuant to Executive Order N-40-20 and an additional 60 calendar days pursuant to Executive Order N-66-20.

27. Amendment of subsections (a)(1)(A) and (a)(7), repealer of subsection (a)(7)(B), subsection relettering, amendment of Table C-5, subsection (d)(1), Table D-4, subsections (d)(2) and (d)(4), Table D-11, subsections (d)(5)-(6), Table F-5, Table G-2, subsections (j)(2)(D), (k)(2), (k)(2)(B), (k)(3)(B), (k)(4)(B), (k)(5)(B) and (l), repealer of subsections (l)(1)-(2), amendment of subsections (n)(2)(C) and (s)(4), amendment of Table T-4 and subsection (x) filed 3-16-2021; operative 3-16-2021 pursuant to Government Code section 11343.4(b)(3) (Register 2021, No. 12). (Filing deadline specified in Government Code section 11349.3(a) extended 60 calendar days pursuant to Executive Order N-40-20.)

28. Change without regulatory effect amending subsections (g)(7)(A) and (u)(1) - Table U-1 filed 7-12-2021 pursuant to section 100, title 1, California Code of Regulations (Register 2021, No. 29).

29. Amendment filed 7-18-2024; operative 7-18-2024 pursuant to Government Code section 11343.4(b)(3) (Register 2024, No. 29).

This database is current through 12/6/24 Register 2024, No. 49.

Cal. Admin. Code tit. 20, § 1605.1, 20 CA ADC § 1605.1