General service incandescent lamp

means a standard incandescent or halogen type lamp that is intended for general service applications; has a medium screw base; has a lumen range of not less than 310 lumens and not more than 2,600 lumens or, in the case of a modified spectrum lamp, not less than 232 lumens and not more than 1,950 lumens; and is capable of being operated at a voltage range at least partially within 110 and 130 volts; however this definitiondoes not apply to the following incandescent lamps—

(1) an appliance lamp;

(2) a black light lamp;

(3) a bug lamp;

(4) a colored lamp;

(5) a G shape lamp with a diameter of 5 inches or more as defined in ANSI C79.1-2002;

(6) an infrared lamp;

(7) a left-hand thread lamp;

(8) a marine lamp;

(9) a marine signal service lamp;

(10) a mine service lamp;

(11) a plant light lamp;

(12) an R20 short lamp;

(13) a sign service lamp;

(14) a silver bowl lamp;

(15) a showcase lamp; and

(16) a traffic signal lamp.