Vibration service lamp

means a lamp that:

(1) has filament configurations that are C‐5, C‐7A, or C‐9, as listed in Figure 6‐12 of the 9th Edition of the IES Lighting Handbook or similar configurations;

(2) has a maximum wattage of 60 watts;

(3) is sold at retail in packages of two lamps or less; and

(4) is designated and marketed specifically for vibration service or vibration‐resistant applications with:

(A) the designation appearing on the lamp packaging; and

(B) marketing materials that identify the lamp as being vibration service only.

1602 (l)