Colored incandescent lamp

means an incandescent lamp designated and marketed as a colored lamp that has:

(1) a CRI of less than 50, as determined according to the test method given in CIE publication 13.3‐1995; or

(2) a correlated color temperature less than 2,500K, or greater than 4,600K, where correlated color temperature is computed according to the Journal of Optical Society of America, Vol. 58, pages 1528‐1595 (1968).