Composite video

means a video display interface that uses Radio Corporation of America (RCA) connections carrying a signal defined by the Society of Motion Picture and Television Engineers' (SMPTE) standard, SMPTE 170M-2004 for regions that support a power frequency of 59.94 Hz or International Telecommunication Union's (ITU) standard, ITU-R BT 470-6 for regions that support a power frequency of 50 Hz.