Two-speed dedicated-purpose pool pump

means a dedicated-purpose pool pump that is capable of operating at only two different pre-determined operating speeds, where the low operating speed is less than or equal to half of the maximum operating speed and greater than zero, and is distributed in commerce either:

(A) with a pool pump control (e.g., variable speed drive and user interface or switch) that is capable of changing the speed in response to user preferences; or

(B) without a pool pump control that has the capability to change speed in response to user preferences, but is unable to operate without the presence of such a pool pump control.