Built-in compact cooler

means any cooler with a total refrigerated volume less than 7.75 ft3 and no more than 24 inches in depth, excluding doors, handles, and custom front panels, that is designed, intended, and marketed exclusively to be:

(1) installed totally encased by cabinetry or panels that are attached during installation;

(2) securely fastened to adjacent cabinetry, walls or floor;

(3) equipped with unfinished sides that are not visible after installation; and

(4) equipped with an integral factory-finished face or built to accept a custom front panel.