General purpose electric motor (subtype II)

means any general purpose electric motors which incorporates design elements of a general purpose electric motor (subtype I) but, unlike a general purpose electric motor (subtype I), is configured in one or more of the following ways:

(1) is built in accordance with NEMA U‐frame dimensions as described in NEMA MG1‐ 1967 or in accordance with the IEC metric equivalents, including a frame size that is between two consecutive NEMA frame sizes or their IEC metric equivalents;

(2) performance in accordance with NEMA Design C characteristics as described in NEMA MG1 – 2009 or an equivalent IEC design(s) such as IEC Design H;

(3) is a close‐coupled pump motor;

(4) is a footless motor;

(5) is a vertical solid shaft normal thrust motor (as tested in a horizontal configuration) built and designed in a manner consistent with NEMA MG1‐2009;

(6) is an eight‐pole motor (900 RPM); or

(7) is a polyphase motor with a voltage rating of not more than 600 volts, is not rated at 230 or 460 volts (or both), and cannot be operated on 230 or 460 volts (or both).