Air curtain unit

means equipment that produces a directionally controlled stream of air with a minimum width-to-depth aspect ratio of 5:1 and a discharge that is not intended to be connected to unitary ductwork. The controlled stream of air spans the entire height and width of an opening and reduces the infiltration or transfer of air from one side of the opening to the other and/or inhibits the passage of insects, dust, or debris.