Colored lamp

means a colored fluorescent lamp, a colored incandescent lamp, or a lamp designed and marketed as a colored lamp with either of the following characteristics (if multiple modes of operation are possible [such as variable CCT], either of the below characteristics must be maintained throughout all modes of operation):

(1) a CRI less than 40, as determined according to the method set forth in CIE Publication 13.3; or

(2) a CCT less than 2,500K or greater than 7,000K.