Federally‐regulated incandescent reflector lamp

(commonly referred to as a reflector lamp) means any lamp in which light is produced by a filament heated to incandescence by an electric current, that:

(1) is not colored or designed for rough or vibration service applications;

(2) contains an inner reflective coating on the outer bulb to direct the light;

(3) has an R, PAR, ER, BR, BPAR, or similar bulb shape with an E26 medium screw base;

(4) has a rated voltage or voltage range that lies at least partially in the range of 115 and 130 volts;

(5) has a diameter that exceeds 2.25 inches; and

(6) has a rated wattage that is 40 watts or higher.