Enhanced-performance display (EPD)

means a computer monitor that has all of the following features and functionalities:

(1) A contrast ratio of at least 60:1 measured at a horizontal viewing angle of at least 85o, with or without a screen cover glass;

(2) A native resolution equal to or greater than 2.3 megapixels (MP); and

(3) A color gamut size of at least sRGB as defined by IEC 61966-2 - 1:1999. Shifts in color space are allowable as long as 99 percent or more of defined sRGB colors are supported.